{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":12,"n_cols":4,"rows_kept":12,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L1"]
[]
[]
[]
[]
["","","","FDXS50F2VEB9 / RXS50L2V1B1"]
["Capacitate de răcire","Nom.","kW","4.80 (1)"]
["Eficienţă nominală","EER","","3.37"]
["","COP","","3.29"]
["Capacitate de încălzire","Nom.","kW","5.80 (2)"]
["Note","","","(1) - Temperatură interioară: 27°C termometru uscat, 19°C termometru umed; temperatură exterioară: 35°C termometru uscat, 24°C termometru umed"]
["","","","(2) - Temperatură interioară: 20°C termometru uscat, 15°C termometru umed; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed."]