{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","38"]
["","","Medie","dBA","36"]
["","","Scăzut","dBA","30"]
["","Răcire","Medie","dBA","36"]
["","","Scăzut","dBA","30"]
["","","Înalt","dBA","38"]
["Accesorii standard","Manual de instalare","","","1"]
["","Manual de utilizare","","","1"]
["","Izolaţie pentru montaj","","","1"]
["","Plăcuţă de etanşare","","","1"]
["","Clemă metalică","","","1"]
["","Furtun de drenare","","","1"]
["","Şaibă pentru consola suportului","","","8"]
["","Material de etanşare","","","2"]
["","Cleme","","","6"]
["","Placă fixare şaibă","","","4"]
["","Şuruburi pentru flanşele tubulaturii","","","1"]
["","Filtru de aer","","","1"]
["Racorduri conducte","Lichid","Dext","mm","6.35"]
["","Gaz","Dext","mm","12.7"]
["","Drenare","","","VP20 (I.D. 20/O.D. 26)"]
["Putere intrare","Răcire","Nom.","kW","0.060"]
["","Încălzire","Nom.","kW","0.060"]
["Sound power level","Răcire","","dBA","55"]
["","Încălzire","","dBA","55"]
["Dimensiuni","Unitate","Lățime","mm","1,150"]
["","","Adâncime","mm","620"]
["","","Înălțime","mm","200"]
["Greutate","Unitate","","kg","30.0"]
["Ventilator","Presiune statică externă","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frecvenţă","","Hz","50/60"]
["","Nume","","","VE"]
["","Tensiune","","V","220-240"]
["Note","","","","(1) - Atunci când sunteţi conectat la aparatul exterior al unui multisistem, consultaţi specificaţiile unităţii multi exterioară de conectat."]