{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Carcasă","Material","","","","Tablă din oţel galvanizat","Tablă din oţel galvanizat","Tablă din oţel galvanizat","Tablă din oţel galvanizat"]
["Dimensiuni","Unitate","","Înălțime","mm","260","260","260","260"]
["","","","Lățime","mm","575","575","575","575"]
["","","","Adâncime","mm","575","575","575","575"]
["Greutate","Unitate","","","kg","16.0","16.0","17.5","17.5"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","9.0","10.0","12.0","14.5"]
["","","","Medie","m³/min","8.0","8.5","10.0","12.5"]
["","","","Scăzut","m³/min","6.5","6.5","7.5","9.5"]
["","","Încălzire","Înalt","m³/min","9.0","10.0","12.0","14.5"]
["","","","Medie","m³/min","8.0","8.5","10.0","12.5"]
["","","","Scăzut","m³/min","6.5","6.5","7.5","9.5"]
["Nivel de putere sonoră","Răcire","","","dBA","48","51","56","60"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","31.0","34.0","39.0","43.0"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","28.5","30.5","34.0","40.0"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","25.0","25.0","27.0","32.0"]
["","Încălzire","","Înalt","dBA","31.0","34.0","39.0","43.0"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","28.5","30.5","34.0","40.0"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","25.0","25.0","27.0","32.0"]
["Racorduri conducte","Lichid","","Dext","mm","6.35","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","9.52","9.52","12.70","12.70"]
["","Drenare","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Panou decorativ","Model","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Culoare","","","","Alb (N9.5)","Alb (N9.5)","Alb (N9.5)","Alb (N9.5)"]
["","Dimensiuni","","Înălțime","mm","46","46","46","46"]
["","","","Lățime","mm","620","620","620","620"]
["","","","Adâncime","mm","620","620","620","620"]
["","Greutate","","","kg","2.8","2.8","2.8","2.8"]
["Panou decorativ 2","Model","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Culoare","","","","Argintiu","Argintiu","Argintiu","Argintiu"]
["","Dimensiuni","","Înălțime","mm","46","46","46","46"]
["","","","Lățime","mm","620","620","620","620"]
["","","","Adâncime","mm","620","620","620","620"]
["","Greutate","","","kg","2.8","2.8","2.8","2.8"]
["Panou decorativ 3","Model","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Culoare","","","","Alb (RAL9010)","Alb (RAL9010)","Alb (RAL9010)","Alb (RAL9010)"]
["","Dimensiuni","","Înălțime","mm","55","55","55","55"]
["","","","Panou decorativ 3-=-Dimensiuni-=-Lățime-=-mm","mm","700","700","700","700"]
["","","","Adâncime","mm","700","700","700","700"]
["","Greutate","","","kg","2.7","2.7","2.7","2.7"]
["Panou decorativ 4","Model","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Culoare","","","","Alb (RAL9010)","Alb (RAL9010)","Alb (RAL9010)","Alb (RAL9010)"]
["","Dimensiuni","","Înălțime","mm","55","55","55","55"]
["","","","Lățime","mm","700","700","700","700"]
["","","","Adâncime","mm","700","700","700","700"]
["","Greutate","","","kg","2.7","2.7","2.7","2.7"]
["Sisteme de control","Telecomandă cu infraroșii","","","","BRC7EB530 (panou standard), BRC7F530W (panou alb), BRC7F530S (panou gri)","BRC7EB530 (panou standard), BRC7F530W (panou alb), BRC7F530S (panou gri)","BRC7EB530 (panou standard), BRC7F530W (panou alb), BRC7F530S (panou gri)","BRC7EB530 (panou standard), BRC7F530W (panou alb), BRC7F530S (panou gri)"]
["","Telecomandă cu fir","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Accesorii standard","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240"]