{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZAG-B"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / RZAG35B5V1B","FFA50A2VEB9 / RZAG35B5V1B","FFA50A2VEB9 / RZAG50B5V1B","FFA60A2VEB9 / RZAG50B5V1B","FFA60A2VEB9 / RZAG60B5V1B"]
["Capacitate de răcire","Capacitate de răcire-=-Min.-=-kW","","kW","1.6","1.6","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","5","5","6"]
["","Max.","","kW","4.5","4.5","6","6","6.5"]
["Capacitate de încălzire","Min.","","kW","1.4","1.4","1.5","1.5","1.6"]
["","Nom.","","kW","4","4","5.8","5.8","7"]
["","Max.","","kW","5","5","6","6","7.5"]
["Eficienţă nominală","EER","","","4","4.25","3.4","3.62","3.23"]
["","COP","","","3.71","3.94","3.1","3.15","2.9"]
["","Consum anual de energie","","kWh","438","412","735","691","929"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A","A","A"]
["","","Încălzire","","A","A","D","D","D"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","A++","A++","A++","A++","A+"]
["","Capacitate","Pdesign","kW","3.5","3.5","5","5","6"]
["","SEER","","","6.4","6.81","6.3","6.43","5.8"]
["","Consum anual de energie","","kWh/a","191","180","278","272","362"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","A","A+","A+","A+","A+"]
["","Capacitate","Pdesign","kW","4.2","4.2","4.3","4.3","4.5"]
["","SCOP/A","","","3.8","4.04","4.01","4.08","4.04"]
["","Pdh Capacitate de încălzire la -10 °","","kW","3.5","3.53","3.66","3.68","3.87"]
["","Consum anual de energie","","kWh/a","1546","1455","1501","1474","1558"]