{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Capacitate de răcire","Nom.","","kW","3.40"]
["Răcire a spațiului","SEER","","","6.24"]
["","Consum anual de energie","","kWh/a","191"]
["","Capacitate","Pdesign","kW","3.40"]
["","Clasă de eficienţă energetică","","","A++"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Clasă de eficienţă energetică","","","A+"]
["","Consum anual de energie","","kWh/a","979"]
["Eficienţă nominală","Consum anual de energie","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Directiva privind clasificarea energetică","Răcire","","A"]
["","","Încălzire","","A"]
["Capacitate de încălzire","Nom.","","kW","4.00"]
["Note","","","","(1) - Vezi desenele separate pentru datele electrice"]
["","","","","(2) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","(3) - Capacităţile nom. de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","(4) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["Outdoor unit","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Capacitate de răcire","Nom.","","kW","","5.00","5.70"]
["Capacitate de încălzire","Nom.","","kW","","6.00","7.20"]
["Eficienţă nominală","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Consum anual de energie","","kWh","","780","867"]
["","Directiva privind clasificarea energetică","Răcire","","","B","A"]
["","","Încălzire","","","C","C"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","","A+","A+"]
["","Capacitate","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Consum anual de energie","","kWh/a","","295","328"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","","A","A"]
["","Capacitate","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Capacitate de încălzire la -10 °","","kW","","3.85","4.08"]
["","Consum anual de energie","","kWh/a","","1578","1704"]