{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Medie","dBA","31","32","33","34"]
["","Răcire","Medie","dBA","34","35","35","36"]
["","","Scăzut","dBA","31","32","33","34"]
["","","Înalt","dBA","36","37","37","38"]
["Accesorii standard","Tub cu izolaţie termică","","","2","2","2","2"]
["","Material pentru agrafe din sârmă","","","7","7","7","7"]
["","Bandă furtun","","","1","1","1","1"]
["","Furtun de drenare","","","1","1","1","1"]
["","Şaibă","","","8","8","8","8"]
["","Plăcuţă de etanşare (mare)","","","1","1","1","1"]
["","Plăcuţă de etanşare (mică)","","","1","1","1","1"]
["","Bucşă din răşină","","","1","1","1","1"]
["","Şuruburi","","","2","2","2","2"]
["","Armătură cabluri","","","2","2","2","2"]
["Sisteme de control","Wired remote control","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Racorduri conducte","Lichid","Dext","mm","6.35","6.35","6.35","9.52"]
["","Gaz","Dext","mm","9.50","12.7","12.7","15.9"]
["","Drain","","","VP20","VP20","VP20","VP20"]
["Sound power level","Răcire","","dBA","53","54","54","55"]
["Dimensiuni","Unitate","Lățime","mm","960","960","1,270","1,270"]
["","","Adâncime","mm","690","690","690","690"]
["","","Înălțime","mm","235","235","235","235"]
["Carcasă","Material","","","Răşină, foaie din metal","Răşină, foaie din metal","Răşină, foaie din metal","Răşină, foaie din metal"]
["","Culoare","","","Alb","Alb","Alb","Alb"]
["Greutate","Unitate","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Fază","","","1~","1~","1~","1~"]
["","Frecvenţă","","Hz","50","50","50","50"]
["","Tensiune","","V","220-240","220-240","220-240","220-240"]
["Note","","","","(1) - Vezi desenele separate pentru datele electrice","(1) - Vezi desenele separate pentru datele electrice","(1) - Vezi desenele separate pentru datele electrice","(1) - Vezi desenele separate pentru datele electrice"]