{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Capacitate de răcire","Min.","","kW","1.2"]
["","Max.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Racorduri conducte","Lichid","Dext","mm","6.35"]
["","Gaz","Dext","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Eficienţă nominală","Consum anual de energie","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Directiva privind clasificarea energetică","Răcire","","B"]
["","","Încălzire","","B"]
["Capacitate de încălzire","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - 220V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240V"]
["","","","","(5) - Răcire: temperatură interioară: 27°C termometru uscat, 19.0°C termometru umed; temperatură exterioară 35 °C termometru uscat; 24°C termometru umed; lungime echivalentă tubulatură: 5m"]
["","","","","(6) - Încălzire: temperatură interioară: 20°C termometru uscat; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed; lungime echivalentă traseu agent frigorific: 5m"]
["","","","","(7) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]