{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L3"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L3V1B"]
["Capacitate de răcire","Nom.","","kW","3.5 (2)"]
["Piping connections","Lichid","Dext","mm","6.35"]
["","Gaz","Dext","mm","9.5"]
["","Drain","OD","mm","18.0"]
["Eficienţă nominală","Consum anual de energie","","kWh","608"]
["","EER","","","2.88 (1)"]
["","COP","","","3.57 (1)"]
["","Directiva privind clasificarea energetică","Răcire","","B"]
["","","Încălzire","","A"]
["Capacitate de încălzire","Nom.","","kW","4.0 (2)"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]
["","","","","(3) - 220V"]
["","","","","(4) - 230 V"]
["","","","","(5) - 240V"]