{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","46"]
["","","Funcţionare silenţioasă","dBA","30"]
["","","Scăzut","dBA","33"]
["","Răcire","Funcţionare silenţioasă","dBA","29"]
["","","Scăzut","dBA","32"]
["","","Înalt","dBA","38"]
["","","Nom.","dBA","36"]
["","Răcire","Nom.","dBA","35"]
["Accesorii standard","Manual de instalare","","","1"]
["","Manual de utilizare","","","1"]
["","Telecomandă prin infraroşu","","","1"]
["","Baterii uscate AAA","","","2"]
["","Suport telecomandă","","","1"]
["","Placă de montare","","","1"]
["","Tub izolant termic (conductă agent frigorific)","","","8"]
["","Filtru de purificare a aerului","","","1"]
["","Filtru dezodorizant fotocatalitic","","","1"]
["","Capac lateral","","","2"]
["","Bandă de îmbinare","","","4"]
["Sisteme de control","Infrared remote control","","","ARC433B67"]
["Piping connections","Lichid","Dext","mm","6.35"]
["","Gaz","Dext","mm","9.5"]
["","Drenare","","","18"]
["Nivel de putere sonoră","Răcire","","dBA","53"]
["","Încălzire","","dBA","59"]
["Dimensiuni","Unitate","Lățime","mm","1,050"]
["","","Adâncime","mm","200"]
["","","Înălțime","mm","490"]
["Carcasă","Colour","","","Alb migdală"]
["Greutate","Unitate","","kg","16"]
["Power supply","Phase","","","1~"]
["","Frecvenţă","","Hz","50"]
["","Nume","","","VM"]
["","Tensiune","","V","220-240"]
["Note","","","","(1) - 220V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240V"]
["","","","","(4) - Atunci când sunteţi conectat la aparatul exterior al unui multisistem, consultaţi specificaţiile unităţii multi exterioară de conectat."]