{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","39","40","41","","46"]
["","","","Medie","dBA","32","33","33","","42"]
["","","","Funcţionare silenţioasă","dBA","19","19","19","","24"]
["","","","Scăzut","dBA","25","25","25","","33"]
["","Răcire","","Medie","dBA","32","33","33","","39"]
["","","","Funcţionare silenţioasă","dBA","19","19","19","","24"]
["","","","Scăzut","dBA","25","25","25","","31"]
["","","","Înalt","dBA","39","40","41","","46"]
["Accesorii standard","Manual de instalare","","","","1","1","1","","1"]
["","Manual de utilizare","","","","1","1","1","","1"]
["","Filtru de aer","","","","2","2","2","","2"]
["","Telecomandă prin infraroşu","","","","1","1","1","","1"]
["","Placă de montare telecomandă","","","","1","1","1","","1"]
["","Pungă şuruburi","","","","1","1","1","","1"]
["","Capac şuruburi","","","","1","1","1","","1"]
["","Baterii uscate AAA","","","","2","2","2","","2"]
["","Măsuri generale privind siguranţa","","","","1","1","1","","1"]
["Agent frigorific","GWP","","","","675.0","675.0","675.0","","675.0"]
["Sisteme de control","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Racorduri conducte","Lichid","","Dext","mm","6.35","6.35","6.35","","6.35"]
["","Gaz","","Dext","mm","9.50","9.50","9.50","","12.70"]
["","Drenare","","","","18","18","18","","18"]
["Putere intrare","Răcire","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Încălzire","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Nivel de putere sonoră","Răcire","","","dBA","57","57","60","","60"]
["Dimensiuni","Unitate","","Lățime","mm","798","798","798","","798"]
["","","","Adâncime","mm","189","189","189","","189"]
["","","","Înălțime","mm","295","295","295","","295"]
["Carcasă","Colour","","","","Alb","Alb","Alb","","Alb"]
["Greutate","Unitate","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Medium","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Scăzut","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Funcţionare silenţioasă","m³/min","4.5","4.5","4.5","","5.7"]
["","","Răcire","Scăzut","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Medium","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Înalt","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Funcţionare silenţioasă","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Phase","","","","1~","1~","1~","","1~"]
["","Nume","","","","V1","V1","V1","","V1"]
["","Frecvenţă","","","Hz","50","50","50","","50"]
["","Tensiune","","","V","220-240","220-240","220-240","","220-240"]
["Putere intrare","Răcire","","Nom.","kW","","","","0.028"]
["","Încălzire","","Nom.","kW","","","","0.036"]
["Carcasă","Culoare","","","","","","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","","","295"]
["","","","Lățime","mm","","","","798"]
["","","","Adâncime","mm","","","","189"]
["Greutate","Unitate","","","kg","","","","11.50"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","","","13.1"]
["","","","Medie","m³/min","","","","9.8"]
["","","","Scăzut","m³/min","","","","7.2"]
["","","","Funcţionare silenţioasă","m³/min","","","","4.6"]
["","","Încălzire","Înalt","m³/min","","","","14.6"]
["","","","Medie","m³/min","","","","10.5"]
["","","","Scăzut","m³/min","","","","7.7"]
["","","","Funcţionare silenţioasă","m³/min","","","","5.2"]
["Nivel de putere sonoră","Răcire","","","dBA","","","","60"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","45"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","","","37"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","","","29"]
["","","","Funcţionare silenţioasă","dBA","","","","21"]
["","Încălzire","","Înalt","dBA","","","","45"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","","","37"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","","","29"]
["","","","Funcţionare silenţioasă","dBA","","","","21"]
["Agent frigorific","GWP","","","","","","","675.0"]
["Racorduri conducte","Lichid","","Dext","mm","","","","6.35"]
["","Gaz","","Dext","mm","","","","12.70"]
["","Drenare","","","","","","","18"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","","ARC466A58"]
["","Telecomandă cu fir","","","","","","","BRC073"]
["Accesorii standard","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Filtru de aer","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Alimentare electrică","Nume","","","","","","","V1"]
["","Fază","","","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","","50"]
["","Tensiune","","","V","","","","220-240"]