{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BB / RXA-A"]
[]
[]
[]
[]
["","","","","FTXA20B2V1BB / RXA20A5V1B","FTXA20B2V1BB / RXA20A3V1B","FTXA25B2V1BB / RXA25A5V1B","FTXA25B2V1BB / RXA25A3V1B","FTXA35B2V1BB / RXA35A5V1B","FTXA35B2V1BB / RXA35A3V1B"]
["Capacitate de răcire","Min.","","kW","1.3","1.3","1.3","1.3","1.4","1.4"]
["","Max.","","kW","2.6","2.6","3.2","3.2","4.0","4.0"]
["","Nom.","","kW","2.0","2.0","2.5","2.5","3.4","3.4"]
["Eficienţă nominală","EER","","","4.70","4.70","4.46","4.46","4.37","4.37"]
["","COP","","","5.00","5.00","5.00","5.00","4.04","4.04"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A","A","A","A"]
["","","Încălzire","","A","A","A","A","A","A"]
["Capacitate de încălzire","Nom.","","kW","2.50","2.50","2.80","2.80","4.00","4.00"]
["","Min.","","kW","1.30","1.30","1.30","1.30","1.40","1.40"]
["","Max.","","kW","3.50","3.50","4.70","4.70","5.20","5.20"]
["Outdoor unit","","","","","RXA20A2V1B","","RXA25A2V1B","","RXA35A2V1B"]