{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":7,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-BB / RXA-A9"]
[]
[]
[]
[]
["","","","","FTXA20B2V1BB / RXA20A5V1B9","FTXA25B2V1BB / RXA25A5V1B9","FTXA35B2V1BB / RXA35A5V1B9"]
["Unitate exterioară","","","","RXA20A5V1B9","RXA25A5V1B9","RXA35A5V1B9"]
["Capacitate de răcire","Capacitate de răcire-=-Min.-=-kW","","kW","1.30","1.30","1.40"]
["","Nom.","","kW","2.00","2.50","3.40"]
["","Max.","","kW","2.60","3.20","4.00"]
["Capacitate de încălzire","Min.","","kW","1.30","1.30","1.40"]
["","Nom.","","kW","2.50","2.80","4.00"]
["","Max.","","kW","3.50","4.70","5.20"]
["Eficienţă nominală","EER","","","4.70","4.46","4.37"]
["","COP","","","5.00","5.00","4.04"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A"]
["","","Încălzire","","A","A","A"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","A+++","A+++","A+++"]
["","Capacitate","Pdesign","kW","2.00","2.50","3.40"]
["","SEER","","","8.75","8.74","8.73"]
["","Consum anual de energie","","kWh/a","80","100","136"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","A+++","A+++","A+++"]
["","Capacitate","Pdesign","kW","2.40","2.45","2.50"]
["","SCOP/A","","","5.15","5.15","5.15"]
["","Pdh Capacitate de încălzire la -10 °","","kW","2.19","2.30","2.36"]
["","Consum anual de energie","","kWh/a","653","666","680"]
["Domeniu de eficiență energetică","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]