{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-C"]
[]
[]
[]
[]
["","","","","","FTXC20CV1B","FTXC25CV1B","FTXC35CV1B","FTXC50CV1B","FTXC60CV1B","FTXC71CV1B"]
["Nivelul de presiune sonoră","Răcire","","Medie","dBA","33","33","34","39","42","42"]
["","","","Funcţionare silenţioasă","dBA","20","20","21","29","30","30"]
["","","","Scăzut","dBA","26","26","26","33","38","38"]
["","","","Înalt","dBA","38","38","39","45","46","46"]
["Sisteme de control","Infrared remote control","","","","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2","ARC486A2"]
["Racorduri ţevi","Lichid","","Dext","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","9.52","9.52","9.52","12.7","12.7","12.7"]
["","Drenare","","","","16.5","16.5","16.5","16.5","16.5","16.5"]
["Putere absorbită","Răcire","","Nom.","kW","0.595","0.765","1.05","1.55","1.89","2.38"]
["","Încălzire","","Nom.","kW","0.670","0.750","1.07","1.52","1.68","2.46"]
["Sound power level","Răcire","","","dBA","54","54","55","57","60","60"]
["Dimensiuni","Unitate","","Lățime","mm","770","770","770","770","990","990"]
["","","","Adâncime","mm","234","234","234","234","273","273"]
["","","","Înălțime","mm","288","288","288","288","297","297"]
["Carcasă","Material","","","","Polistiren rezistent la şoc","Polistiren rezistent la şoc","Polistiren rezistent la şoc","Polistiren rezistent la şoc","Polistiren rezistent la şoc","Polistiren rezistent la şoc"]
["","Culoare","","","","Alb","Alb","Alb","Alb","Alb","Alb"]
["Greutate","Unitate","","","kg","9.00","9.00","9.50","9.50","13.0","13.0"]
["Ventilator","Debit de aer","Răcire","Scăzut","m³/min","6.5","6.5","6.5","8.2","13.6","13.6"]
["","","","Medium","m³/min","9","9","9","10","16","16"]
["","","","Înalt","m³/min","10.8","10.8","10.8","12.2","20.4","20.4"]
["","","","Funcţionare silenţioasă","m³/min","5.4","5.4","5.4","7.4","10.2","10.2"]
["Power supply","Fază","","","","1~","1~","1~","1~","1~","1~"]
["","Frecvenţă","","","Hz","50","50","50","50","50","50"]
["","Nume","","","","V1","V1","V1","V1","V1","V1"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]