{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":10,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-E / RXC-E"]
[]
[]
[]
[]
["","","","","FTXC20EV1B / RXC20EV1B","FTXC25EV1B / RXC25EV1B","FTXC35EV1B / RXC35EV1B","FTXC50EV1B / RXC50EV1B","FTXC60EV1B / RXC60EV1B","FTXC71EV1B / RXC71EV1B"]
["Outdoor unit","","","","RXC20EV1B","RXC25EV1B","RXC35EV1B","RXC50EV1B","RXC60EV1B","RXC71EV1B"]
["Capacitate de răcire","Capacitate de răcire-=-Min.-=-kW","","kW","1.3","1.3","1.3","1.37","1.8","2.3"]
["","Max.","","kW","3.0","3.0","4.0","6.2","7.0","7.3"]
["Capacitate de încălzire","Min.","","kW","1.3","1.3","1.3","1.36","1.48","2.3"]
["","Max.","","kW","4.0","4.0","4.8","6.6","8.0","9.0"]
["Eficienţă nominală","EER","","","3.36","3.35","3.35","3.29","3.30","2.98"]
["","COP","","","3.73","3.79","3.74","3.71","3.81","3.25"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A","A","A","C"]
["","","Încălzire","","A","A","A","A","A","C"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","A++","A++","A++","A++","A++","A"]
["","Capacitate","Pdesign","kW","2.1","2.6","3.4","5.1","6.2","7.0"]
["","SEER","","","6.9","6.8","6.9","6.5","6.4","5.3"]
["","Consum anual de energie","","kWh/a","106","131","175","276","339","460"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","A+","A+","A+","A+","A+","A"]
["","Capacitate","Pdesign","kW","1.9","2.2","2.2","3.9","4.1","6.4"]
["","SCOP/A","","","4.4","4.5","4.3","4.4","4.2","3.8"]
["","Pdh Capacitate de încălzire la -10 °","","kW","1.4","1.6","1.7","3.0","3.5","5.4"]
["","Consum anual de energie","","kWh/a","595","701","733","1234","1353","2332"]