{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","39","40"]
["","","Medie","dBA","34","34"]
["","","Funcţionare silenţioasă","dBA","21","21"]
["","","Scăzut","dBA","28","28"]
["","Răcire","Medie","dBA","33","33"]
["","","Funcţionare silenţioasă","dBA","20","20"]
["","","Scăzut","dBA","25","26"]
["","","Înalt","dBA","39","40"]
["Accesorii standard","Manual de instalare","","","1","1"]
["","Manual de utilizare","","","1","1"]
["","Telecomandă prin infraroşu","","","1","1"]
["","Baterii uscate AAA","","","2","2"]
["","Suport telecomandă","","","1","1"]
["","Placă de montare","","","1","1"]
["","Şuruburi de fixare a aparatului interior","","","2","2"]
["Sisteme de control","Telecomandă cu fir","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Racorduri ţevi","Lichid","Dext","mm","6.35","6.35"]
["","Gaz","Dext","mm","9.50","9.50"]
["","Drenare","","","18","18"]
["Putere intrare","Răcire","Nom.","kW","0.017","0.019"]
["","Încălzire","Nom.","kW","0.020","0.020"]
["Nivel de putere sonoră","Răcire","","dBA","55","55"]
["","Încălzire","","dBA","55","55"]
["Dimensiuni","Unitate","Lățime","mm","770","770"]
["","","Adâncime","mm","225","225"]
["","","Înălțime","mm","286","286"]
["Carcasă","Culoare","","","Alb","Alb"]
["Greutate","Unitate","","kg","8.50","8.50"]
["Power supply","Fază","","","1~","1~"]
["","Frecvenţă","","Hz","50","50"]
["","Tensiune","","V","220-240","220-240"]