{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":7,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-E"]
[]
[]
[]
[]
["","","","","","FTXF20E5V1B","FTXF42E5V1B"]
["Putere intrare","Răcire","","Nom.","kW","0.023","0.040"]
["","Încălzire","","Nom.","kW","0.023","0.040"]
["Carcasă","Culoare","","","","Alb","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","286","286"]
["","","","Lățime","mm","770","770"]
["","","","Adâncime","mm","225","225"]
["Greutate","Unitate","","","kg","8","9.00"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","9.8","12.6"]
["","","","Medie","m³/min","8","9"]
["","","","Scăzut","m³/min","6","6.9"]
["","","","Funcţionare silenţioasă","m³/min","4.3","4.9"]
["","","Încălzire","Înalt","m³/min","10.4","12.8"]
["","","","Medie","m³/min","8.3","8.8"]
["","","","Scăzut","m³/min","6.2","6.7"]
["","","","Funcţionare silenţioasă","m³/min","5.3","5.2"]
["Nivel de putere sonoră","Răcire","","","dBA","53","59.0"]
["","Încălzire","","","dBA","55","59.0"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","39","45.0"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","33","36.0"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","25","30.0"]
["","","","Funcţionare silenţioasă","dBA","20","22.0"]
["","Încălzire","","Înalt","dBA","39","44.0"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","34","34.0"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","28","28.0"]
["","","","Funcţionare silenţioasă","dBA","21","22.0"]
["Racorduri conducte","Lichid","","Dext","mm","6","6"]
["","Gaz","","Dext","mm","9.5","9.50"]
["","Drenare","","","","18","18"]
["Sisteme de control","Telecomandă cu infraroșii","","","","ARC470A1","ARC470A1"]
["","Telecomandă cu fir","","","","BRC073A1","BRC073A1"]
["Accesorii standard","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-440","220-440"]