{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXG-LW / RXLG-M"]
[]
[]
[]
[]
["","","","","FTXG25LV1BW / RXLG25M2V1B","FTXG35LV1BW / RXLG35M2V1B"]
["Capacitate de răcire","Min.","","kW","1.3","1.4"]
["","Max.","","kW","4.0","4.6"]
["","Nom.","","kW","2.5 (2)","3.5 (2)"]
["Racorduri ţevi","Lichid","Dext","mm","6.35","6.35"]
["","Gaz","Dext","mm","9.5","9.5"]
["","Drenare","Dext","mm","18","18"]
["Eficienţă nominală","Consum anual de energie","","kWh","340","490"]
["","EER","","","3.68 (1)","3.57 (1)"]
["","COP","","","4.31 (1)","3.89 (1)"]
["","Directiva privind clasificarea energetică","Răcire","","A","A"]
["","","Încălzire","","A","A"]
["Capacitate de încălzire","Nom.","","kW","4.4 (2)","5.1 (2)"]
["","Min.","","kW","1.0 (6)","1.0 (6)"]
["","Max.","","kW","6.1, 3.6 (7)","6.7, 4.2 (7)"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]
["","","","","(3) - 220V","(3) - 220V"]
["","","","","(4) - 230 V","(4) - 230 V"]
["","","","","(5) - 240V","(5) - 240V"]
["","","","","(6) - Pentru capacitatea minimă nominală de încălzire, ventilatorul unităţii interioare este setat la SL","(6) - Pentru capacitatea minimă nominală de încălzire, ventilatorul unităţii interioare este setat la SL"]
["","","","","(7) - Capacitate maximă de încălzire la o temperatură exterioară de -15°C","(7) - Capacitate maximă de încălzire la o temperatură exterioară de -15°C"]