{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":9,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AS / RXJ-A"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BS / RXJ20A5V1B","FTXJ25A2V1BS / RXJ25A5V1B","FTXJ35A2V1BS / RXJ35A5V1B","FTXJ42A2V1BS / RXJ42A2V1B","FTXJ50A2V1BS / RXJ50A2V1B"]
["Outdoor unit","","","","RXJ20A5V1B","RXJ25A5V1B","RXJ35A5V1B","RXJ42A2V1B","RXJ50A2V1B"]
["Capacitate de răcire","Capacitate de răcire-=-Min.-=-kW","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Nom.","","kW","2.0","2.5","3.4","4.2","5.0"]
["","Max.","","kW","2.6","3.2","4.0","5.0","5.3"]
["Capacitate de încălzire","Min.","","kW","1.3","1.3","1.4","1.7","1.7"]
["","Nom.","","kW","2.5","2.8","4.0","5.4","5.8"]
["","Max.","","kW","3.5","4.7","5.2","6.0","6.5"]
["Eficienţă nominală","EER","","","4.7","4.46","4.37","3.99","3.68"]
["","COP","","","5.0","5.0","4.04","4.12","4.0"]
["","Consum anual de energie","","kWh","213","280","389","526","679"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A","A","A"]
["","","Încălzire","","A","A","A","A","A"]
["Răcirea spaţiului","Clasă de eficienţă energetică","","","A+++","A+++","A+++","A++","A++"]
["","Capacitate","Pdesign","kW","2.0","2.5","3.4","4.2","5.0"]
["","SEER","","","8.75","8.74","8.73","7.5","7.33"]
["","Consum anual de energie","","kWh/a","80","100","136","196","239"]
["Încălzirea spaţiului (climat temperat)","Clasă de eficienţă energetică","","","A+++","A+++","A+++","A++","A++"]
["","Capacitate","Pdesign","kW","2.4","2.45","2.5","3.8","4.0"]
["","SCOP/A","","","5.15","5.15","5.15","4.6","4.6"]
["","Pdh Capacitate de încălzire la -10 °","","kW","2.02","2.07","2.11","3.26","3.44"]
["","Consum anual de energie","","kWh/a","652","666","680","1,156","1,218"]