{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","38","39","42","42","44","","46"]
["","","","Funcţionare silenţioasă","dBA","25","25","26","30","31","","34"]
["","","","Scăzut","dBA","28","28","29","33","34","","37"]
["","Răcire","","Funcţionare silenţioasă","dBA","22","22","23","30","31","","34"]
["","","","Scăzut","dBA","25","25","26","33","34","","37"]
["","","","Înalt","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Răcire","","Nom.","dBA","32","32","34","38","39","","42"]
["Accesorii standard","Filtru pentru purificarea aerului din apatit de titan fotocatalitic","","","","2","2","2","2","2"]
["","Manual de utilizare","","","","1","1","1","1","1","","1"]
["","Manual de instalare","","","","1","1","1","1","1","","1"]
["","Telecomandă fără fir","","","","1","1","1","1","1","","1"]
["","Baterii","","","","2","2","2","2","2","","2"]
["","Suport telecomandă","","","","1","1","1","1","1","","1"]
["","Şuruburi de fixare a aparatului interior","","","","2","2","2","2","2","","2"]
["","Placă de montare","","","","1","1","1","1","1","","1"]
["Sisteme de control","Infrared remote control","","","","","","","","","","ARC452A3"]
["Racorduri ţevi","Liquid","","Dext","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gaz","","Dext","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Drenare","","","","18","18","18","18","18","","18"]
["Putere absorbită","Răcire","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Încălzire","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Nivel de putere sonoră","Răcire","","","dBA","54","54","58","58","59","","63"]
["","Încălzire","","","dBA","54","55","58","58","60","","62"]
["Dimensiuni","Unitate","","Lăţime","mm","800","800","800","800","800","","1,050"]
["","","","Adâncime","mm","215","215","215","215","215","","250"]
["","","","Înălţime","mm","295","295","295","295","295","","290"]
["Carcasă","Culoare","","","","Alb","Alb","Alb","Alb","Alb","","Alb"]
["Weight","Unitate","","","kg","9","9","10","10","10","","12"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frecvenţă","","","Hz","50","50","50","50","50","","50"]
["","Nume","","","","V1","V1","V1","V1","V1","","V1"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - SL: Nivelul silenţios la reglarea debitului de aer la ventilator"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230 V"]
["Ventilator","Debit de aer","Răcire","Nom.","m³/min","","","","","","16.0"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","","","","","","41"]
["Ventilator","Debit de aer","Încălzire","Nom.","m³/min","","","","","","14.9"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","","","","","","40"]
["Putere intrare","Răcire","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Încălzire","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Carcasă","Culoare","","","","","","","","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","","","","","290"]
["","","","Lățime","mm","","","","","","1050"]
["","","","Adâncime","mm","","","","","","250"]
["Greutate","Unitate","","","kg","","","","","","12"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","","","","","16.0"]
["","","","Scăzut","m³/min","","","","","","11.3"]
["","","","Funcţionare silenţioasă","m³/min","","","","","","10.1"]
["","","Încălzire","Înalt","m³/min","","","","","","17.2"]
["","","","Scăzut","m³/min","","","","","","12.6"]
["","","","Funcţionare silenţioasă","m³/min","","","","","","11.3"]
["Nivel de putere sonoră","Răcire","","","dBA","","","","","","60"]
["","Încălzire","","","dBA","","","","","","59"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","","","45"]
["","","","Scăzut","dBA","","","","","","36"]
["","","","Funcţionare silenţioasă","dBA","","","","","","33"]
["","Încălzire","","Înalt","dBA","","","","","","44"]
["","","","Scăzut","dBA","","","","","","35"]
["","","","Funcţionare silenţioasă","dBA","","","","","","32"]
["Racorduri conducte","Lichid","","Dext","mm","","","","","","6.35"]
["","Gaz","","Dext","mm","","","","","","12.7"]
["","Drenare","","","","","","","","","18"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","","","","ARC452A3"]
["Accesorii standard","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Alimentare electrică","Nume","","","","","","","","","V1"]
["","Fază","","","","","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","","","","50"]
["","Tensiune","","","V","","","","","","220-240"]
["Accesorii standard","Filtru pentru purificarea aerului din apatit de titan fotocatalitic fără cadru","","","","","","","","","","2"]
["Note","","","","","","","","","","","(4) - 240V"]