{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L3"]
[]
[]
[]
[]
["","","","","FTXS20K3V1B / RXS20L3V1B","FTXS20K2V1B / RXS20L3V1B","FTXS25K3V1B / RXS25L3V1B","FTXS25K2V1B / RXS25L3V1B","FTXS35K2V1B / RXS35L3V1B","FTXS35K3V1B / RXS35L3V1B"]
["Capacitate de răcire","Min.","","kW","","","","","","1.4"]
["","Max.","","kW","","","","","","4.0"]
["","Nom.","","kW","2.00 (2)","2.0","2.5 (2)","2.5","3.5","3.5 (2)"]
["Racorduri conducte","Lichid","Dext","mm","6.35","","6.35","","","6.35"]
["","Gaz","Dext","mm","9.5","","9.5","","","9.5"]
["","Drenare","OD","mm","18","","18","","","18"]
["Eficienţă nominală","Consum anual de energie","","kWh","228","228","297","297","450","450"]
["","EER","","","4.39 (1)","4.39","4.21 (1)","4.21","3.89","3.89 (1)"]
["","COP","","","4.72 (1)","4.72","4.67 (1)","4.67","4.76","4.76 (1)"]
["","Directiva privind clasificarea energetică","Răcire","","A","A","A","A","A","A"]
["","","Încălzire","","A","A","A","A","A","A"]
["Capacitate de încălzire","Nom.","","kW","2.5 (2)","2.5","2.8 (2)","2.8","4.0","4.00 (2)"]
["","Min.","","kW","1.3","","1.3","","","1.4"]
["","Max.","","kW","4.3","","4.7","","","5.2"]
["Note","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]
["","","","","(3) - 220V","","(3) - 220V","","","(3) - 220V"]
["","","","","(4) - 230 V","","(4) - 230 V","","","(4) - 230 V"]
["","","","","(5) - 240V","","(5) - 240V","","","(5) - 240V"]