{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","41"]
["","","","Medie","dBA","31"]
["","","","Funcţionare silenţioasă","dBA","19"]
["","","","Scăzut","dBA","24"]
["","Răcire","","Medie","dBA","32"]
["","","","Funcţionare silenţioasă","dBA","20"]
["","","","Scăzut","dBA","25"]
["","","","Înalt","dBA","43"]
["Accesorii standard","Manual de instalare","","","","1"]
["","Manual de utilizare","","","","1"]
["","Filtru de aer","","","","2"]
["","Telecomandă prin infraroşu","","","","1"]
["","Placă de montare telecomandă","","","","1"]
["","Pungă şuruburi","","","","1"]
["","Capac şuruburi","","","","2"]
["","Baterii uscate AAA","","","","2"]
["","Măsuri generale privind siguranţa","","","","1"]
["Agent frigorific","GWP","","","","675.0"]
["Sisteme de control","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Piping connections","Lichid","","Dext","mm","6.35"]
["","Gaz","","Dext","mm","9.50"]
["","Drain","","","","18"]
["Putere absorbită","Răcire","","Nom.","kW","0.023"]
["","Încălzire","","Nom.","kW","0.022"]
["Nivel de putere sonoră","Răcire","","","dBA","60"]
["","Încălzire","","","dBA","60"]
["Dimensiuni","Unitate","","Lățime","mm","798"]
["","","","Adâncime","mm","189"]
["","","","Înălțime","mm","295"]
["Carcasă","Colour","","","","Negru."]
["Greutate","Unitate","","","kg","11.5"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","11.5"]
["","","","Scăzut","m³/min","6.0"]
["","","","Medie","m³/min","8.0"]
["","","","Funcţionare silenţioasă","m³/min","5.1"]
["","","Răcire","Scăzut","m³/min","5.7"]
["","","","Medie","m³/min","8.3"]
["","","","Înalt","m³/min","11.9"]
["","","","Funcţionare silenţioasă","m³/min","4.6"]
["Power supply","Fază","","","","1~"]
["","Frecvenţă","","","Hz","50"]
["","Nume","","","","V1"]
["","Tensiune","","","V","220-240"]
["Note","","","","","(1) - Răcire: temperatură interioară: 27°C termometru uscat, 19.0°C termometru umed; temperatură exterioară 35 °C termometru uscat; 24°C termometru umed; lungime echivalentă tubulatură: 5m"]
["","","","","","(2) - Încălzire: temperatură interioară: 20°C termometru uscat; temperatură exterioară: 7°C termometru uscat, 6°C termometru umed; lungime echivalentă traseu agent frigorific: 5m"]
["","","","","","(3) - Vezi desenele separate pentru datele electrice"]