{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BB"]
["Putere intrare","Răcire","","Nom.","kW","0.023"]
["","Încălzire","","Nom.","kW","0.022"]
["Carcasă","Culoare","","","","Negru."]
["Dimensiuni","Unitate","","Înălțime","mm","295"]
["","","","Lățime","mm","798"]
["","","","Adâncime","mm","189"]
["Greutate","Unitate","","","kg","12"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","13.1"]
["","","","Medie","m³/min","9"]
["","","","Scăzut","m³/min","6"]
["","","","Funcţionare silenţioasă","m³/min","4.9"]
["","","Încălzire","Înalt","m³/min","12.3"]
["","","","Medie","m³/min","8.2"]
["","","","Scăzut","m³/min","5.8"]
["","","","Funcţionare silenţioasă","m³/min","5"]
["Nivel de putere sonoră","Răcire","","","dBA","60"]
["","Încălzire","","","dBA","60"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","43"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","32"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","25"]
["","","","Funcţionare silenţioasă","dBA","20"]
["","Încălzire","","Înalt","dBA","41"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","31"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","24"]
["","","","Funcţionare silenţioasă","dBA","19"]
["Agent frigorific","GWP","","","","675"]
["Racorduri conducte","Lichid","","Dext","mm","6.35"]
["","Gaz","","Dext","mm","9.5"]
["","Drenare","","","","18"]
["Sisteme de control","Telecomandă cu infraroșu","","","","ARC466A84"]
["Sisteme de control","Telecomandă cu fir","","","","BRC073A4"]
["Accesorii standard","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","220-240"]