{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","43"]
["","","","Medie","dBA","35"]
["","","","Funcţionare silenţioasă","dBA","21"]
["","","","Scăzut","dBA","26"]
["","Răcire","","Medie","dBA","35"]
["","","","Funcţionare silenţioasă","dBA","21"]
["","","","Scăzut","dBA","26"]
["","","","Înalt","dBA","43"]
["Accesorii standard","Manual de instalare","","","","1"]
["","Manual de utilizare","","","","1"]
["","Telecomandă fără fir","","","","1"]
["","Baterii uscate AAA","","","","2"]
["","Suport telecomandă","","","","1"]
["","Placă de montare","","","","1"]
["","Filtru de dezodorizare din apatit de titan","","","","2"]
["","Şuruburi de fixare a aparatului interior","","","","2"]
["Sisteme de control","Telecomandă cu fir","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Racorduri ţevi","Lichid","","Dext","mm","6.35"]
["","Gaz","","Dext","mm","9.50"]
["","Drenare","","","","16 (diametru interior al furtunului de conectare)"]
["Putere absorbită","Răcire","","Nom.","kW","0.030"]
["","Încălzire","","Nom.","kW","0.035"]
["Sound power level","Răcire","","","dBA","58"]
["","Încălzire","","","dBA","58"]
["Dimensiuni","Unitate","","Lățime","mm","770"]
["","","","Adâncime","mm","225"]
["","","","Înălțime","mm","285"]
["Carcasă","Culoare","","","","Alb"]
["Greutate","Unitate","","","kg","9.0"]
["Power supply","Fază","","","","1~"]
["","Frecvenţă","","","Hz","50"]
["","Nume","","","","V1"]
["","Tensiune","","","V","220-240"]
["Note","","","","","(1) - Vezi desenele separate pentru datele electrice"]
["Putere intrare","Răcire","","Nom.","kW","","0.03"]
["","Încălzire","","Nom.","kW","","0.035"]
["Carcasă","Culoare","","","","","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","285"]
["","","","Lățime","mm","","770"]
["","","","Adâncime","mm","","225"]
["Greutate","Unitate","","","kg","","9"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","11.4"]
["","","","Medie","m³/min","","8.2"]
["","","","Scăzut","m³/min","","5.4"]
["","","","Funcţionare silenţioasă","m³/min","","4.3"]
["","","Încălzire","Înalt","m³/min","","10.8"]
["","","","Medie","m³/min","","7.8"]
["","","","Scăzut","m³/min","","5.8"]
["","","","Funcţionare silenţioasă","m³/min","","4.9"]
["Nivel de putere sonoră","Răcire","","","dBA","","58"]
["","Încălzire","","","dBA","","58"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","43"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","35"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","26"]
["","","","Funcţionare silenţioasă","dBA","","21"]
["","Încălzire","","Înalt","dBA","","43"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","35"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","26"]
["","","","Funcţionare silenţioasă","dBA","","21"]
["Racorduri conducte","Lichid","","Dext","mm","","6.35"]
["","Gaz","","Dext","mm","","9.5"]
["","Drenare","","","","","16 (diametru interior al furtunului de conectare)"]
["Sisteme de control","Infrared remote control","","","","","ARC480A11"]
["Sisteme de control","Telecomandă cu fir","","","","","BRC944B2, BRC073A1"]
["Accesorii standard","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Alimentare electrică","Nume","","","","","V1"]
["","Fază","","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","50"]
["","Tensiune","","","V","","220-240"]