{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","39","42","44"]
["","","","Funcţionare silenţioasă","dBA","19","19","24"]
["","","","Scăzut","dBA","28","29","31"]
["","Răcire","","Funcţionare silenţioasă","dBA","19","19","23"]
["","","","Scăzut","dBA","26","27","30"]
["","","","Înalt","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Răcire","","Nom.","dBA","33","35","38"]
["Accesorii standard","Filtru fotocatalitic de purificare şi dezodorizare a aerului","","","","1","1","1"]
["","Telecomandă fără fir","","","","1","1","1"]
["","Baterii uscate","","","","2","2","2"]
["","Suport telecomandă","","","","1","1","1"]
["","Şuruburi de fixare a aparatului interior","","","","3","3","3"]
["","Placă de montare","","","","1","1","1"]
["Control systems","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Racorduri conducte","Lichid","","Dext","mm","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","9.5","9.5","9.5"]
["Putere intrare","Răcire","","Nom.","kW","0.030","0.030","0.030"]
["","Încălzire","","Nom.","kW","0.030","0.030","0.030"]
["Nivel de putere sonoră","Răcire","","","dBA","54","57","60"]
["","Încălzire","","","dBA","56","57","59"]
["Dimensiuni","Unitate","","Lățime","mm","798","798","798"]
["","","","Adâncime","mm","372","372","372"]
["","","","Înălțime","mm","295","295","295"]
["Carcasă","Colour","","","","Alb","Alb","Alb"]
["Greutate","Unitate","","","kg","15","15","15"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","11.7","13.3","14.4"]
["","","","Scăzut","m³/min","6.7","6.9","7.7"]
["","","","Funcţionare silenţioasă","m³/min","4.8","4.8","5.9"]
["","","Răcire","Scăzut","m³/min","5.3","5.6","6.6"]
["","","","Înalt","m³/min","10.7","12.1","15.0"]
["","","","Funcţionare silenţioasă","m³/min","4.0","4.0","4.6"]
["","","","Nom.","m³/min","8.6","9.2","10.7"]
["","","Răcire","Nom.","m³/min","7.5","8.4","9.2"]
["Power supply","Phase","","","","1~","1~","1~"]
["","Nume","","","","V1","V1","V1"]
["","Frecvenţă","","","Hz","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Partea frontală a schimbătorului de căldură","(4) - Partea frontală a schimbătorului de căldură","(4) - Partea frontală a schimbătorului de căldură"]
["","","","","","(5) - Partea posterioară a schimbătorului de căldură","(5) - Partea posterioară a schimbătorului de căldură","(5) - Partea posterioară a schimbătorului de căldură"]