{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":12,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Domeniu de eficiență energetică","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Capacitate de răcire","Nom.","","kW","","","","","","","","6.80"]
["Răcire a spaţiului","SEER","","","","","","","","","","6.42"]
["","Consum anual de energie","","kWh/a","","","","","","","","371"]
["","Capacitate","Pdesign","kW","","","","","","","","6.80"]
["","Clasă de eficienţă energetică","","","","","","","","","","A++"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","","","","","","","","7.60"]
["","SCOP/A","","","","","","","","","","4.20"]
["","Clasă de eficienţă energetică","","","","","","","","","","A+"]
["","Consum anual de energie","","kWh/a","","","","","","","","2,534"]
["Eficienţă nominală","Consum anual de energie","","kWh","","","","","","","","835"]
["","EER","","","","","","","","","","4.07"]
["","COP","","","","","","","","","","4.08"]
["","Directiva privind clasificarea energetică","Răcire","","","","","","","","","A"]
["","","Încălzire","","","","","","","","","A"]
["Capacitate de încălzire","Nom.","","kW","","","","","","","","7.50"]
["Note","","","","","","","","","","","(1) - Capacităţile nominale de răcire se bazează pe: temperatură interioară: 27 °CDB, 19 °CWB, temperatură exterioară: 35 °CDB, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","","","","","","","","(2) - Capacităţile nominale de încălzire se bazează pe: temperatură interioară: 20°C termometru uscat, temperatura exterioară: 7°C termometru uscat, 6°C termometru umed, lungime echivalentă traseu agent frigorific: 5 m, diferenţă de nivel: 0 m."]
["","","","","","","","","","","","(3) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","","","","","","","","(4) - Vezi desenele separate pentru datele electrice"]