{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","","","","41","46","47"]
["","","","Medie","dBA","","","","38","42","43"]
["","","","Scăzut","dBA","","","","35","39","40"]
["","Răcire","","Medie","dBA","","","","38","42","43"]
["","","","Scăzut","dBA","","","","35","39","40"]
["","","","Înalt","dBA","","","","41","46","47"]
["Accesorii standard","Manual de utilizare","","","","","","","1","1","1"]
["","Manual de instalare","","","","","","","1","1","1"]
["","Furtun de drenare","","","","","","","1","1","1"]
["","Tub cu izolaţie termică","","","","","","","3","3","3"]
["","Legături","","","","","","","10","10","10"]
["","Bandă furtun","","","","","","","1","1","1"]
["","Material de etanşare","","","","","","","4","4","4"]
["","Placă fixare şaibă","","","","","","","1","1","1"]
["","Racord de drenare","","","","","","","1","1","1"]
["","Material neţesut","","","","","","","1","1","1"]
["","Şaibă","","","","","","","8","8","8"]
["","Şurub de fixare pentru furtunul de drenare","","","","","","","5","5","5"]
["Sisteme de control","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Capacitate de răcire","Capacitate totală","","Nom.","kW","","","","","","12.1"]
["Racorduri conducte","Lichid","","Dext","mm","","","","9.52","9.52","9.52"]
["","Gaz","","Dext","mm","","","","15.9","15.9","15.9"]
["","Drenare","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Răcire","","","dBA","","","","59","64","65"]
["","Încălzire","","","dBA","","","","59","64"]
["Dimensiuni","Unitate","","Lățime","mm","","","","950","950","950"]
["","","","Adâncime","mm","","","","950","950","950"]
["","","","Înălțime","mm","","","","198","198","198"]
["Carcasă","Material","","","","","","","Răşină","Răşină","Răşină"]
["","Culoare","","","","","","","Alb crud","Alb crud","Alb crud"]
["Greutate","Unitate","","","kg","","","","25.0","26.0","26"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Scăzut","m³/min","","","","16.0","20.0","20.5"]
["","","Răcire","Scăzut","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Înalt","m³/min","","","","23.0","31.0","32.5"]
["Înălțime de drenare","mm","","","","","","","600","600","600"]
["Capacitate de încălzire","Capacitate totală","","Nom.","kW","","","","","","13.5"]
["Carcasă","Culoare","","","","Alb crud","Alb crud","Alb crud"]
["","Material","","","","Răşină","Răşină","Răşină"]
["Dimensiuni","Unitate","","Înălțime","mm","198","198","198"]
["","","","Lățime","mm","950","950","950"]
["","","","Adâncime","mm","950","950","950"]
["Greutate","Unitate","","","kg","25.0","26.0","26.0"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","23.0","31.0","32.5"]
["","","","Medie","m³/min","19.5","25.5","26.5"]
["","","","Scăzut","m³/min","16.0","20.0","20.5"]
["","","Încălzire","Înalt","m³/min","23.0","31.0","32.5"]
["","","","Medie","m³/min","19.5","25.5","26.5"]
["","","","Scăzut","m³/min","16.0","20.0","20.5"]
["Nivel de putere sonoră","Răcire","","","dBA","59","64","65"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","41","46","47"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","38","42","43"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","35","39","40"]
["","Încălzire","","Înalt","dBA","41","46","47"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","38","42","43"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","35","39","40"]
["Racorduri conducte","Lichid","","Dext","mm","9.52","9.52","9.52"]
["","Gaz","","Dext","mm","15.9","15.9","15.9"]
["","Drenare","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Înălțime de drenare","mm","","","","600","600","600"]
["Accesorii standard","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Capacitate de răcire","Capacitate totală","","Nom.","kW","","","12.10"]
["Capacitate de încălzire","Capacitate totală","","Nom.","kW","","","13.5"]