{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":10,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ71CVEB / RZQG71L8Y1B","FVQ100CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Capacitate de răcire","Nom.","","kW","6.8","","","","12.0","13.4"]
["Răcire a spaţiului","SEER","","","6.23","6.31","5.61","5.61","5.61"]
["","Consum anual de energie","","kWh/a","383","378","593","749","748.663"]
["","Capacitate","Pdesign","kW","6.80","6.80","9.50","12.00","12.00"]
["","Clasă de eficienţă energetică","","","A++","A++","A+","A+","A+"]
["Încălzirea spaţiului (climat temperat)","Capacitate","Pdesign","kW","6.33","6.33","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","3.87","3.87"]
["","Clasă de eficienţă energetică","","","A+","A+","A+","A","A"]
["","Consum anual de energie","","kWh/a","2,189","2,189","3,767","4,088","4,087.855"]
["Eficienţă nominală","Consum anual de energie","","kWh","1,010","","","","1,870","2,085"]
["","EER","","","3.37","","","","3.21","3.21"]
["","COP","","","3.64","","","","3.70","3.61"]
["","Directiva privind clasificarea energetică","Răcire","","A","","","","A"]
["","","Încălzire","","A","","","","A"]
["Capacitate de încălzire","Nom.","","kW","7.5","","","","13.5","15.5"]
["Note","","","","(1) - Consumul anual de energie este în conformitate cu Directiva 2002/31/CE privind etichetarea consumului de energie","","","","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE","(1) - EER/COP conform Eurovent 2012, pentru utilizare numai în afara UE"]
["","","","","(2) - SEER şi SCOP sunt în conformitate cu EN 14825","","","","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°","(2) - Eficienţă nominală: răcire la o sarcină nominală de 35°/27°, încălzire la o sarcină nominală de 7°/20°"]