{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Nivelul de presiune sonoră","Încălzire","Înalt","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Scăzut","dBA","38","44","46","48"]
["","Răcire","Scăzut","dBA","38","44","46","48"]
["","","Înalt","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Accesorii standard","Manual de utilizare","","","Manual de utilizare","Manual de utilizare","Manual de utilizare","Manual de utilizare"]
["","Manual de instalare","","","Manual de instalare","Manual de instalare","Manual de instalare","Manual de instalare"]
["","Suport pentru montaj","","","Suport pentru montaj","Suport pentru montaj","Suport pentru montaj","Suport pentru montaj"]
["","Cauciuc de protecţie pentru orificii","","","Cauciuc de protecţie pentru orificii","Cauciuc de protecţie pentru orificii","Cauciuc de protecţie pentru orificii","Cauciuc de protecţie pentru orificii"]
["","Perie","","","Perie","Perie","Perie","Perie"]
["","Izolaţie pentru montaj","","","Izolaţie pentru montaj","Izolaţie pentru montaj","Izolaţie pentru montaj","Izolaţie pentru montaj"]
["","Capac","","","Capac","Capac","Capac","Capac"]
["","Cleme","","","Cleme","Cleme","Cleme","Cleme"]
["","Şuruburi","","","Şuruburi","Şuruburi","Şuruburi","Şuruburi"]
["","Model de instalare","","","Model de instalare","Model de instalare","Model de instalare","Model de instalare"]
["","Material rezistent la vaporizare","","","Material rezistent la vaporizare","Material rezistent la vaporizare","Material rezistent la vaporizare","Material rezistent la vaporizare"]
["","Cablaj telecomandă","","","Cablaj telecomandă","Cablaj telecomandă","Cablaj telecomandă","Cablaj telecomandă"]
["Sisteme de control","Telecomandă cu fir","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Racorduri conducte","Lichid","Dext","mm","9.52","9.52","9.52","9.52"]
["","Gaz","Dext","mm","15.9","15.9","15.9","15.9"]
["","Drenare","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Power input","Răcire","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Încălzire","Nom.","kW","0.117","0.238","0.238","0.276"]
["Nivel de putere sonoră","Răcire","","dBA","55","62","63","65"]
["","Încălzire","","dBA","55","62","63","65"]
["Dimensiuni","Unitate","Lățime","mm","600","600","600","600"]
["","","Adâncime","mm","270","350","350","350"]
["","","Înălțime","mm","1,850","1,850","1,850","1,850"]
["Carcasă","Culoare","","","Alb crud","Alb crud","Alb crud","Alb crud"]
["Greutate","Unitate","","kg","39","47","47","47"]
["Power supply","Fază","","","1~","1~","1~","1~"]
["","Frecvenţă","","Hz","50/60","50/60","50/60","50/60"]
["","Tensiune","","V","220-240/220","220-240/220","220-240/220","220-240/220"]