{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMQ-A"]
[]
[]
[]
[]
["","","","","","FXMQ200AXVMB","FXMQ250AXVMB"]
["Capacitate de răcire","Capacitate totală","","La viteză mare a ventilatorului","kW","22.4","28.0"]
["Capacitate de încălzire","Capacitate totală","","La viteză mare a ventilatorului","kW","25.0","31.5"]
["Putere absorbită - 50 Hz","Răcire","","La viteză mare a ventilatorului","kW","0.54","0.65"]
["","Încălzire","","La viteză mare a ventilatorului","kW","0.54","0.65"]
["Dimensiuni","Unitate","","Înălțime","mm","470","470"]
["","","","Lățime","mm","1490","1490"]
["","","","Adâncime","mm","1100","1100"]
["Greutate","Unitate","","","kg","105","115"]
["Carcasă","Culoare","","","","Nevopsit","Nevopsit"]
["","Material","","","","Tablă din oţel galvanizat","Tablă din oţel galvanizat"]
["Ventilator","Debit de aer - 50 Hz","Răcire","La viteză mare a ventilatorului","m³/min","62","74"]
["","","","La viteză mică a ventilatorului","m³/min","41","52"]
["","Presiune statică externă - 50 Hz","","Mare","Pa","250","250"]
["","","","Scăzută","Pa","50","50"]
["","Presiune statică externă - 60 Hz","","Mare","Pa","250","250"]
["","","","Scăzută","Pa","50","50"]
["Agent frigorific","Tip","","","","R-410A","R-410A"]
["","GWP","","","","2087.5","2087.5"]
["Nivel de putere sonoră","Răcire","","La viteză mare a ventilatorului","dBA","75.0","76.0"]
["Nivel de presiune sonoră","Răcire","","La viteză mare a ventilatorului","dBA","48.0","48.0"]
["","","","La viteză medie a ventilatorului","dBA","46.5","46.5"]
["","","","La viteză mică a ventilatorului","dBA","45.0","45.0"]
["","Încălzire","","La viteză mare a ventilatorului","dBA","48.0","48.0"]
["","","","La viteză medie a ventilatorului","dBA","46.5","46.5"]
["","","","La viteză mică a ventilatorului","dBA","45.0","45.0"]
["Racorduri conducte","Lichid","","Tip","","Racord cu mufă","Racord cu mufă"]
["","","","Dext","mm","9.5","9.5"]
["","Gaz","","Tip","","Flanşă","Flanşă"]
["","","","Dext","mm","19.1","22.2"]
["","Drenare","","","","BSP1","BSP1"]
["Accesorii standard","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","1","1"]
["","Spring washer","","","","2","2"]
["","Hexagon head screw","","","","2","2"]
["","Plain washer","","","","8","8"]
["","Hexagon head screw with washer","","","","49","49"]
["","Gas connection pipe","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["Alimentare electrică","Nume","","","","VM","VM"]
["","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50/60","50/60"]
["","Tensiune","","","V","220-240/220-230","220-240/220-230"]
["Curent - 50 Hz","Curent maxim la siguranțe (MFA)","","","A","6","6"]