{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK555A"]
[]
[]
[]
[]
["","","","","","MCK555AVM-W"]
["Tip","","","","","Purificator de aer cu umidificator"]
["Aplicaţie","","","","","Unităţi tip de pardoseală"]
["Carcasă","Culoare","","","","Alb (N9. 0)"]
["Dimensiuni","Unitate","","Înălțime","mm","700"]
["","","","Lățime","mm","270"]
["","","","Adâncime","mm","270"]
["Greutate","Unitate","","","kg","9.5"]
["Zona aplicabilă din încăpere","m²","","","","41 (1), 82 (2)"]
["CADR","m³/h","","","","320"]
["Funcţia de purificare a aerului","Putere intrare","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Silenţios","kW","0.007"]
["Funcţia de umidificare","Putere intrare","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Silenţios","kW","0.009"]
["","Capacitatea rezervorului de apă","","","l","2.7"]
["Nivelul de presiune sonoră","Funcţia de purificare a aerului","","Turbo","dBA","53"]
["","","","Mediu","dBA","39"]
["","","","Scăzut","dBA","29"]
["","","","Silenţios","dBA","20"]
["","Funcţia de umidificare","","Turbo","dBA","53"]
["","","","Mediu","dBA","39"]
["","","","Scăzut","dBA","33"]
["","","","Silenţios","dBA","20"]
["Ventilator","Debit de aer","Funcţia de purificare a aerului","Turbo","m³/h","330"]
["","","","Mediu","m³/h","192"]
["","","","Scăzut","m³/h","120"]
["","","","Silenţios","m³/h","54"]
["","","Funcţia de umidificare","Turbo","m³/h","330"]
["","","","Mediu","m³/h","192"]
["","","","Scăzut","m³/h","144"]
["","","","Silenţios","m³/h","54"]
["Metoda de colectare a prafului","","","","","Filtru HEPA electrostatic"]
["Metoda de dezodorizare","","","","","Flash Streamer + catalizator dezodorizant"]
["Accesorii standard","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Remote controller","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["Cablu de alimentare","m","","","","1.8"]
["Alimentare electrică","Fază","","","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50/60"]
["","Tensiune","","","V","220-240/220-230"]
["Note","","","","","(1) - Zona de acoperire este adecvată pentru funcționarea unității la turația maximă a ventilatorului (HH). Zona de acoperire indică spațiul din care o anumită cantitate de particule de praf poate fi eliminată în 30 de minute."]
["","","","","","(2) - Transformate la standardele NRCC de la valorile de test conform JEM1467."]
["","","","","","(3) - Transformate la standardele CADR de la valorile de test conform JEM1467."]
["","","","","","(4) - Volumul de umidificare variază în funcţie de temperatura şi umiditatea interioară şi exterioară. Condiţii de măsurare: o temperatură de 20°C şi o umiditate de 30%."]
["","","","","","(5) - Nivelurile zgomotului în timpul funcționării reprezintă media valorilor măsurate la 1 m distanță față de partea frontală, stângă, dreaptă și de sus a unității. (Aceste valori sunt egale cu valoarea măsurată într-o cameră fără ecou.)"]
["","","","","","(6) - Filtrul HEPA electrostatic și filtrele de umidificare sunt montate în unitate."]
["","","","","","(7) - Cerințe conform JEM1467."]