{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":5,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RTD-RA"]
[]
[]
[]
[]
["","","","","RTD-RA."]
["Temperatura din mediul ambiant","Depozitare","Min.","°C","-10"]
["","","Max.","°C","50"]
["","În timpul funcţionării","Min.","°C","0"]
["","","Max.","°C","50"]
["Dimensiuni","Unitate","Lățime","mm","80"]
["","","Adâncime","mm","37.5"]
["","","Înălțime","mm","80"]
["Power supply","Tensiune","","V","15 V DC"]