{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A9"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B9","RXA25A5V1B9","RXA35A5V1B9"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","550"]
["","","","Lățime","mm","840","840","840"]
["","","","Adâncime","mm","350","350","350"]
["Greutate","Unitate","","","kg","32","32","32"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","46.0","46.0","49.0"]
["","Încălzire","","Nom.","dBA","47.0","47.0","49.0"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32"]
["","Cantitate","","","kg","0.76","0.76","0.76"]
["","Cantitate","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675.0","675.0","675.0"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15.0","15.0","15.0"]
["Accesorii standard","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Alimentare electrică","Fază","","","","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240"]