{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-B"]
[]
[]
[]
[]
["","","","","","RXA42B2V1B","RXA50B2V1B","RXA50B5V1B"]
["Dimensiuni","Unitate","","Înălțime","mm","734","734","734"]
["","","","Lățime","mm","870","870","954"]
["","","","Adâncime","mm","373","373","401"]
["Greutate","Unitate","","","kg","50","50","49"]
["Compressor","Type","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","48.0","48.0","48"]
["","Încălzire","","Nom.","dBA","48.0","48.0","48"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32"]
["","Cantitate","","","kg","1.10","1.10","1.1"]
["","Cantitate","","","tCO2Eq","0.75","0.75","0.75"]
["","GWP","","","","675","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","30","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","20","20","20"]
["Accesorii standard","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Alimentare electrică","Fază","","","","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240"]
["Compresor","Tip","","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Note","","","","","","","(1) - Vezi desenele separate pentru domeniul de funcţionare"]
["","","","","","","","(2) - Vezi desenele separate pentru datele electrice"]
["","","","","","","","(3) - Conţine gaze fluorurate cu efect de seră"]