{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-B"]
[]
[]
[]
[]
["","","","","","RXC20BV1B","RXC25BV1B","RXC35BV1B","RXC50BV1B","RXC60BV1B","RXC71BV1B"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","","","54"]
["Agent frigorific","Charge","","","TCO2Eq","","","","","","0.776"]
["","GWP","","","","","","","","","675"]
["","Încărcare","","","kg","","","","","","1.15"]
["","Tip","","","","","","","","","R-32"]
["Racorduri ţevi","Diferenţa de nivel","IU - OU","Max.","m","","","","","","20.0"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","","","","","","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)"]
["Compresor","Tip","","","","","","","","","Swing ermetic"]
["Dimensiuni","Unitate","","Lățime","mm","","","","","","930"]
["","","","Adâncime","mm","","","","","","350"]
["","","","Înălțime","mm","","","","","","695"]
["Greutate","Unitate","","","kg","","","","","","45"]
["Power supply","Fază","","","","","","","","","1~"]
["","Frecvenţă","","","Hz","","","","","","50"]
["","Tensiune","","","V","","","","","","220-240"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","550","615","615"]
["","","","Lățime","mm","658","658","658","845","845"]
["","","","Adâncime","mm","273","273","273","300","300"]
["Greutate","Unitate","","","kg","24","24","26","39","39"]
["Compresor","Tip","","","","Swing ermetic","Swing ermetic","Swing ermetic","Swing ermetic","Swing ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","10","10","10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","45","45","46","51","54"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32","R-32","R-32"]
["","Cantitate","","","kg","0.55","0.55","0.75","1","1.1"]
["","Cantitate","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743"]
["","GWP","","","","675","675","675","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","20","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)","0,017 (pentru lungimi ale tubulaturii care depăşesc 7,5 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15.0","15.0","15.0","20.0","20.0"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240","220-240"]