{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-D"]
[]
[]
[]
[]
["","","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Nivel de putere sonoră","Răcire","","","dBA","58","58","60","65","66","69"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","550","615","615","695"]
["","","","Lățime","mm","658","658","658","845","845","930"]
["","","","Adâncime","mm","273","273","273","300","300","350"]
["Greutate","Unitate","","","kg","24","24","26","39","39","45"]
["Compresor","Tip","","","","Swing ermetic","Swing ermetic","Swing ermetic","Swing ermetic","Swing ermetic","Swing ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","° C termometru uscat","10","10","10","-10","-10","-10"]
["","","","Max.","° C termometru uscat","46","46","46","46","46","46"]
["","Încălzire","Ambiant","Min.","°C termometru umed","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°C termometru umed","18","18","18","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","45","45","46","51","54","54"]
["Agent frigorific","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Cantitate","","","kg","0.55","0.55","0.75","1","1.1","1.15"]
["","Cantitate","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743","0.776"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","20","30","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)","0017 (pentru lungimi ale tubulaturii care depăşesc 75 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]