{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","","","30.1","30.6","48.9"]
["","","Încălzire","Super scăzută","m³/min","","","25.6","27.2","43.1"]
["","","","Super scăzută","cfm","","","1063","1080","1727"]
["","","Încălzire","Super scăzută","cfm","","","904","960","1522"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","550","550","735"]
["","","","Lățime","mm","765","765","765","765","825"]
["","","","Adâncime","mm","285","285","285","285","300"]
["Greutate","Unitate","","","kg","34","34","34","39","47"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","780","780","780","790","670"]
["","","Încălzire","Super scăzută","rot/min","740","740","740","780","670"]
["Compresor","Type","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46"]
["","Încălzire","Ambiant","Min.","°C termometru umed","-25","-25","-25","-25","-25"]
["","","","Max.","°C termometru umed","18","18","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","46","46","48","48","48"]
["","Încălzire","","Înalt","dBA","47","47","48","48","48"]
["Agent frigorific","Tip","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Cantitate","","","kg","1.0","1.05","1.2","1.3","1.7"]
["","Cantitate","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","20","20","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15","15","15","15","20"]
["Accesorii standard","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Alimentare electrică","Fază","","","","1~","1~","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]