{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","30.6","30.6"]
["","","Încălzire","Super scăzută","m³/min","27.2","27.2"]
["","","","Super scăzută","cfm","1080","1080"]
["","","Încălzire","Super scăzută","cfm","960","960"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550"]
["","","","Lățime","mm","858","858"]
["","","","Adâncime","mm","330","330"]
["Greutate","Unitate","","","kg","40","40"]
["Compressor","Type","","","","","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-25","-25"]
["","","","Max.","°CWB","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","48","48"]
["","","","Scăzut","dBA","44","44"]
["","Încălzire","","Înalt","dBA","49","49"]
["","","","Scăzut","dBA","45","45"]
["Agent frigorific","Tip","","","","R-410A","R-410A"]
["","Cantitate","","","kg","1","1"]
["","Cantitate","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - IU","Max.","m","15","15"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic"]