{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXN-MB"]
[]
[]
[]
[]
["","","","","","RXN25MV1B","RXN35MV1B","RXN50MV1B","RXN60MV1B"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","","","","51"]
["","Răcire","","Nom.","dBA","","","","51"]
["Agent frigorific","Charge","","","TCO2Eq","","","","3"]
["","GWP","","","","","","","2,087.5"]
["","Cantitate","","","kg","","","","1.45"]
["","Tip","","","","","","","R-410A"]
["Compressor","Type","","","","","","","Swing ermetic"]
["Dimensiuni","Unitate","","Lățime","mm","","","","855"]
["","","","Adâncime","mm","","","","328"]
["","","","Înălțime","mm","","","","753"]
["Greutate","Unitate","","","kg","","","","44"]
["Power supply","Phase","","","","","","","1~"]
["","Frecvenţă","","","Hz","","","","50"]
["","Tensiune","","","V","","","","220-240"]
["Note","","","","","","","","(1) - Toate specificaţiile pot fi modificate de către producător fără notificare prealabilă."]
["","","","","","","","","(2) - Conţine gaze fluorurate cu efect de seră"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550","753"]
["","","","Lățime","mm","658","658","855"]
["","","","Adâncime","mm","289","289","328"]
["Greutate","Unitate","","","kg","31","31","44"]
["Compresor","Tip","","","","Swing ermetic","Swing ermetic","Swing ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","10","10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","45","46","51"]
["","Încălzire","","Nom.","dBA","45","46","51"]
["Agent frigorific","Tip","","","","R-410A","R-410A","R-410A"]
["","Cantitate","","","kg","1.00","1.00","1.45"]
["","Cantitate","","","tCO2Eq","2.1","2.1","3"]
["","GWP","","","","2087.5","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20","30"]
["Alimentare electrică","Fază","","","","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240"]