{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","49","","","52"]
["","","","Scăzut","dBA","46","","","49"]
["","Răcire","","Scăzut","dBA","46","","","49"]
["","","","Înalt","dBA","49","","","52"]
["Accesorii standard","Mufă de drenare","","","","1","","","1"]
["","Manual de instalare","","","","1","","","1"]
["Agent frigorific","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Încărcare","","","kg","1.5","","","2.3"]
["","Tip","","","","R-410A","","","R-410A"]
["Racorduri conducte","Diferenţa de nivel","IU - OU","Max.","m","20","","","20"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","","","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["Compresor","Tip","","","","Compresor oscilant etanşat ermetic_","","","Compresor oscilant etanşat ermetic_"]
["Dimensiuni","Unitate","","Lățime","mm","825","","","900"]
["","","","Adâncime","mm","300","","","320"]
["","","","Înălțime","mm","735","","","770"]
["Greutate","Unitate","","","kg","48","","","71"]
["Power supply","Phase","","","","1~","","","1~"]
["","Frecvenţă","","","Hz","50","","","50"]
["","Tensiune","","","V","220-240","","","220-240"]
["Note","","","","","(1) - SL: Nivelul silenţios la reglarea debitului de aer la ventilator","(1) - 220V","","(1) - SL: Nivelul silenţios la reglarea debitului de aer la ventilator","(1) - 220V"]
["","","","","","(2) - Conţine gaze fluorurate cu efect de seră","(2) - 230 V","","(2) - Conţine gaze fluorurate cu efect de seră","(2) - 230 V"]
["Dimensiuni","Unitate","","Înălțime","mm","","735","735","","770","770"]
["","","","Lățime","mm","","825","825","","900","900"]
["","","","Adâncime","mm","","300","300","","320","320"]
["Greutate","Unitate","","","kg","","48","48","","71","71"]
["Compresor","Tip","","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Max.","°CDB","","46","46","","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","","-15","-15","","-15","-15"]
["","","","Max.","°CWB","","18","20","","18","20"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","49","49","","52","52"]
["","","","Scăzut","dBA","","46","46","","49","49"]
["","Încălzire","","Înalt","dBA","","49","49","","52","52"]
["","","","Scăzut","dBA","","46","46","","49","49"]
["Agent frigorific","Tip","","","","","R-410A","R-410A","","R-410A","R-410A"]
["","Cantitate","","","kg","","1.5","1.5","","2.3","2.3"]
["","Cantitate","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","","30","30","","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","","20","20","","20","20"]
["Accesorii standard","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["Alimentare electrică","Fază","","","","","1~","1~","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","50","50","","50","50"]
["","Tensiune","","","V","","220-240","220-240","","220-240","220-240"]
["Note","","","","","","(3) - 240V","","","(3) - 240V"]
["Accesorii standard","Drain socket","","","","","","1","","","1"]
["Nivel de putere sonoră","Răcire","","","dBA","","","","65"]