{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":11,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","47","47","48","48"]
["","Răcire","","Înalt","dBA","46","46","48","48"]
["Accesorii standard","Dop de drenare","","","","1","1","1","1"]
["","Manual de instalare","","","","1","1","1","1"]
["","Etichetă pentru cantitatea de agent frigorific","","","","1","1","1"]
["","Etichete multilingve pentru gaze fluorurate cu efect de seră","","","","1","1","Etichete multilingve pentru gaze fluorurate cu efect de seră"]
["Agent frigorific","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Încărcare","","","kg","1.0","1.0","1.20","1.3"]
["","Tip","","","","R-410A","R-410A","R-410A","R-410A"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","780","780","780","790"]
["","","Încălzire","Super scăzută","rot/min","740","740","740","780"]
["Domeniu de funcţionare","Răcire","Ambiant","Max.","°CDB","46","46","46","46"]
["","","","Min.","°CDB","-10","-10","-10","-10"]
["","Încălzire","Ambiant","Max.","°CWB","18","18","18","18"]
["","","","Min.","°CWB","-15","-15","-15","-15"]
["Racorduri conducte","Diferenţa de nivel","IU - OU","Max.","m","","","15"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","","","0,020 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["Dimensiuni","Unitate","","Lățime","mm","765","765","765","765"]
["","","","Adâncime","mm","285","285","285","285"]
["","","","Înălțime","mm","550","550","550","550"]
["Compresor","Tip","","","","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_"]
["Greutate","Unitate","","","kg","34","34","34","39"]
["Ventilator","Debit de aer","Încălzire","Super scăzută","cfm","904","904","904","960"]
["","","","Super scăzută","m³/min","25.6","25.6","25.6","27.2"]
["","","Răcire","Super scăzută","m³/min","30.1","30.1","30.1","30.6"]
["","","","Super scăzută","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frecvenţă","","","Hz","50","50","50","50"]
["","Tensiune","","","V","220-240","220-240","220-240","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","","","","","48.9","45.0"]
["","","Încălzire","Super scăzută","m³/min","","","","","43.1","46.3"]
["","","","Super scăzută","cfm","","","","","1727","1589"]
["","","Încălzire","Super scăzută","cfm","","","","","1522","1635"]
["Dimensiuni","Unitate","","Înălțime","mm","","","","","735","735"]
["","","","Lățime","mm","","","","","825","825"]
["","","","Adâncime","mm","","","","","300","300"]
["Greutate","Unitate","","","kg","","","","","47","48"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","","","","","670"]
["","","Încălzire","Super scăzută","rot/min","","","","","670"]
["Compresor","Tip","","","","","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","","","","","-10","-10"]
["","","","Max.","°CDB","","","","","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","","","","","-15","-15"]
["","","","Max.","°CWB","","","","","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","","","","48","49"]
["","","","Scăzut","dBA","","","","","44","46"]
["","Încălzire","","Înalt","dBA","","","","","48","49"]
["","","","Scăzut","dBA","","","","","45","46"]
["Agent frigorific","Tip","","","","","","","","R-410A","R-410A"]
["","Cantitate","","","kg","","","","","1.7","1.5"]
["","Cantitate","","","tCO2Eq","","","","","3.5","3.1"]
["","GWP","","","","","","","","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","","","","","30","30"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","","","","","0,020 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,020 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","","","","","20.0","20"]
["Accesorii standard","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Alimentare electrică","Fază","","","","","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","","","","50","50"]
["","Tensiune","","","V","","","","","220-230-240","220-230-240"]
["Note","","","","","","","","","","(1) - 230 V"]