{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","","","48"]
["","Răcire","","Înalt","dBA","","","48"]
["Accesorii standard","Manual de instalare","","","","","","1"]
["","Etichetă pentru cantitatea de agent frigorific","","","","","","1"]
["","Etichete multilingve pentru gaze fluorurate cu efect de seră","","","","","","1"]
["","Dop de drenare (numai pentru modelele cu pompă de căldură)","","","","","","1"]
["Agent frigorific","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Încărcare","","","kg","","","1.2"]
["","Tip","","","","","","R-410A"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","","","780"]
["","","Încălzire","Super scăzută","rot/min","","","740"]
["Domeniu de funcţionare","Răcire","Ambiant","Max.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Încălzire","Ambiant","Max.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Racorduri conducte","Diferenţa de nivel","IU - OU","Max.","m","","","15"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","","","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["Compresor","Tip","","","","","","Compresor oscilant etanşat ermetic_"]
["Dimensiuni","Unitate","","Lățime","mm","","","765"]
["","","","Adâncime","mm","","","285"]
["","","","Înălțime","mm","","","550"]
["Greutate","Unitate","","","kg","","","34"]
["Ventilator","Debit de aer","Încălzire","Super scăzută","cfm","","","904"]
["","","","Super scăzută","m³/min","","","25.6"]
["","","Răcire","Super scăzută","m³/min","","","30.1"]
["","","","Super scăzută","cfm","","","1,063"]
["Power supply","Fază","","","","","","1~"]
["","Frecvenţă","","","Hz","","","50"]
["","Tensiune","","","V","","","220-240"]
["Note","","","","","","","(1) - SL: Nivelul silenţios la reglarea debitului de aer la ventilator"]
["Ventilator","Debit de aer","Răcire","Super scăzută","m³/min","30.1","30.1"]
["","","Încălzire","Super scăzută","m³/min","25.6","25.6"]
["","","","Super scăzută","cfm","1063","1063"]
["","","Încălzire","Super scăzută","cfm","904","904"]
["Dimensiuni","Unitate","","Înălțime","mm","550","550"]
["","","","Lățime","mm","765","765"]
["","","","Adâncime","mm","285","285"]
["Greutate","Unitate","","","kg","34","34"]
["Motor ventilator","Viteză","Răcire","Super scăzută","rot/min","780","780"]
["","","Încălzire","Super scăzută","rot/min","740","740"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Încălzire","Ambiant","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","46","46"]
["","Încălzire","","Înalt","dBA","47","47"]
["Agent frigorific","Tip","","","","R-410A","R-410A"]
["","Cantitate","","","kg","1.0","1.0"]
["","Cantitate","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","20","20"]
["Racorduri ţevi","Încărcare suplimentară de agent frigorific","","","kg/m","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)","0,02 (pentru lungimi ale tubulaturii care depăşesc 10 m)"]
["","Diferenţa de nivel","IU - OU","Max.","m","15","15"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]
["Note","","","","","(1) - 220V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240V"]
["Accesorii standard","Drain plug (only heat pump models)","","","","","1"]