{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","","","48","48","50","50"]
["","Răcire","","Înalt","dBA","","","48","48","49","49"]
["Accesorii standard","Manual de utilizare","","","","","","1","1","1","1"]
["","Manual de instalare","","","","","","1","1","1","1"]
["Agent frigorific","GWP","","","","","","675","675","675","675"]
["","Încărcare","","","kg","","","1.34","1.34","1.34","1.34"]
["","Tip","","","","","","R-32","R-32","R-32","R-32"]
["Domeniu de funcţionare","Răcire","Ambiant","Max.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Încălzire","Ambiant","Max.","°CWB","","","18","18","18","18"]
["","","","Min.","°CWB","","","-20","-20","-20","-20"]
["Racorduri ţevi","Diferenţa de nivel","IU - OU","Max.","m","","","8","8","8","8"]
["Dimensiuni","Unitate","","Lățime","mm","","","795","795","795","795"]
["","","","Adâncime","mm","","","300","300","300","300"]
["","","","Înălțime","mm","","","693","693","693","693"]
["Compresor","Tip","","","","","","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_","Compresor oscilant etanşat ermetic_"]
["Greutate","Unitate","","","kg","","","50","50","50","50"]
["Power supply","Fază","","","","","","1~","1~","1~","1~"]
["","Frecvenţă","","","Hz","","","50","50","50","50"]
["","Tensiune","","","V","","","220-240","220-240","220-240","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră","(4) - Conţine gaze fluorurate cu efect de seră"]
["Dimensiuni","Unitate","","Înălțime","mm","693","693"]
["","","","Lățime","mm","795","795"]
["","","","Adâncime","mm","300","300"]
["Greutate","Unitate","","","kg","50","50"]
["Compresor","Tip","","","","Compresor swing etanşat ermetic","Compresor swing etanşat ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","43","43"]
["","Încălzire","Ambiant","Min.","°CWB","-20","-20"]
["","","","Max.","°CWB","18","18"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","46","46"]
["","Încălzire","","Înalt","dBA","46","46"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","Cantitate","","","kg","1.34","1.34"]
["","Cantitate","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","10","10"]
["Racorduri ţevi","Diferenţa de nivel","IU - OU","Max.","m","8","8"]
["Accesorii standard","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Alimentare electrică","Fază","","","","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","220-240","220-240"]