{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimensiuni","Unitate","","Înălțime","mm","870","870"]
["","","","Lățime","mm","1,100","1,100"]
["","","","Adâncime","mm","460","460"]
["Greutate","Unitate","","","kg","117","117"]
["Compresor","Type","","","","Compresor scroll închis ermetic","Compresor scroll închis ermetic"]
["Domeniu de funcționare","Răcire","Ambiant","Min.","°CDB","-20","-20"]
["","","","Max.","°CDB","46","46"]
["","Încălzire","Ambiant","Min.","°C termometru umed","-20","-20"]
["","","","Max.","°C termometru umed","15","15"]
["Nivel de putere sonoră","Răcire","","","dBA","73","76"]
["","Încălzire","","","dBA","76 (1)","79 (1)"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","53","57"]
["","Încălzire","","Nom.","dBA","60","63"]
["Agent frigorific","Tip","","","","R-32","R-32"]
["","Cantitate","","","kg","5","5"]
["","GWP","","","","675","675"]
["Piping connections","Lichid","","Dext","mm","9.52","9.52"]
["","Gaz","","Dext","mm","22.2","22.2"]
["","Lungime tubulatură","Max.","OU - IU","m","100","100"]
["","","Sistem","Fără încărcare","m","30","30"]
["","Încărcare suplimentară de agent frigorific","","","kg/m","A se vedea manualul de instalare","A se vedea manualul de instalare"]
["Accesorii standard","Manual de instalare","","","","1","1"]
["","Măsuri generale privind siguranţa","","","","1","1"]
["","Legături","","","","2","2"]
["","Etichetă pentru gaze fluorescente, cu dezlipire","","","","1","1"]
["","Racorduri tubulatură","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frecvenţă","","","Hz","50","50"]
["","Tensiune","","","V","380-415","380-415"]
["Curent - 50 Hz","Curent maxim la siguranțe (MFA)","","","A","20","20"]
["Note","","","","","(1) - Măsurat în conformitate cu ENER Lot 21","(1) - Măsurat în conformitate cu ENER Lot 21"]