{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimensiuni","Unitate","","Înălțime","mm","1,680"]
["","","","Lățime","mm","930"]
["","","","Adâncime","mm","765"]
["Greutate","Unitate","","","kg","183.0"]
["Compresor","Type","","","","Compresor scroll închis ermetic"]
["Operation range","Răcire","Ambiant","Min.","°CDB","-5.0"]
["","","","Max.","°CDB","46.0"]
["","Încălzire","Ambiant","Min.","°CWB","-15.0"]
["","","","Max.","°CWB","15.0"]
["Sound power level","Răcire","","","dBA","78.0"]
["","Încălzire","","","dBA","78.0"]
["Agent frigorific","Tip","","","","R-410A"]
["","Cantitate","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Racorduri conducte","Lichid","","Dext","mm","9.52"]
["","Gaz","","Dext","mm","22.2"]
["","Lungime tubulatură","Max.","OU - IU","m","100"]
["","","Sistem","Fără încărcare","m","30"]
["Accesorii standard","Manual de instalare","","","","1"]
["","Racorduri tubulatură","","","","4"]
["Power supply","Fază","","","","3N~"]
["","Frecvenţă","","","Hz","50"]
["","Tensiune","","","V","380-415"]
["Curent - 50 Hz","Curent maxim la siguranțe (MFA)","","","A","25"]
["Note","","","","","(1) - Alimentarea cu tensiune a unităţii interioare FDQ este separată"]
["","","","","","(2) - Vezi desenele separate pentru datele electrice."]
["Dimensiuni","Unitate","","Înălțime","mm","","1680"]
["","","","Lățime","mm","","930"]
["","","","Adâncime","mm","","765"]
["Greutate","Unitate","","","kg","","184.0"]
["Compresor","Tip","","","","","Compresor scroll închis ermetic"]
["Gama de operare","Răcire","Ambiant","Min.","°CDB","","-5.0"]
["","","","Max.","°CDB","","46.0"]
["","Încălzire","Ambiant","Min.","°CWB","","-15.0"]
["","","","Max.","°CWB","","15.0"]
["Nivel de putere sonoră","Răcire","","","dBA","","78.0"]
["","Încălzire","","","dBA","","78.0"]
["Agent frigorific","Cantitate","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["","Cantitate","","","tCO2Eq","","19.4"]
["Racorduri conducte","Lichid","","Dext","mm","","12.70"]
["","Gaz","","Dext","mm","","22.2"]
["Racorduri tubulatură","Lungime tubulatură","Max.","OU - IU","m","","100"]
["Racorduri ţevi","Lungime tubulatură","Sistem","Fără încărcare","m","","30"]
["Accesorii standard","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Alimentare curent","Frecvenţă","","","Hz","","50"]
["Curent - 50 Hz","Curent maxim la siguranțe (MFA)","","","A","","25"]