{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":28,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SP-O"]
[]
[]
[]
[]
["","","","","","MSP106EA12XXA","MSP106EA12XXB","MSP107EA12XXA","MSP107EA12XXB","BSP110DA12XXA","BSP110DA12XXB","BSP112DA12XXA","BSP112DA12XXB","BSP117DA12XXA","BSP117DA12XXB","MSP212EA12XXA","BSP218DA12XXB","BSP218DA12XXA","BSP220DB12XXA","BSP220DB12XXB","MSP315EB13XXA","MSP315EB13XXB","BSP320DB13XXA","BSP320DB13XXB","MSP320EB13XXA","MSP320EB13XXB","BSP330DB13XXA","BSP330DB13XXB"]
["Capacitate de refrigerare","Congelare","R-452A","Nom","kW","","","","","0.662","","0.905","","1.164","","","","1.436","1.719","","","","2.384","","","","2.581"]
["","Temperatură medie","R-134a","Nom","kW","1.14","","1.422","","","","","","","","1.816","","","","","3.188","","","","3.492"]
["Carcasă","Culoare","","Unitate de condensare","","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb","Alb"]
["Dimensiuni","Unitate de condensare","","Lăţime","mm","660","","660","","660","","660","","660","","860","","860","860","","860","","860","","860","","860"]
["","","","Adâncime","mm","337","","337","","337","","337","","337","","427","","427","427","","427","","427","","427","","427"]
["","Unitate evaporator","","Înălţime","mm","","215","","215","","215","","215","","215","","215","","","215","","215","","215","","215","","215"]
["","","","Lăţime","mm","","654","","654","","654","","654","","654","","1074","","","1074","","1654","","1654","","1654","","1654"]
["","","","Adâncime","mm","","410","","410","","410","","410","","410","","410","","","410","","410","","410","","410","","410"]
["Compresor","Cantitate_","","","","1","","1","","1","","1","","1","","1","","1","1","","1","","1","","1","","1"]
["","Tip","","","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori","","Compresor pe bază de vapori"]
["","Model","","","","NJ6220Z","","NTU6222ZV","","NEU2178GK","","NJ2192GK","","NJ2212GK","","FH4518Y/F","","NJ2212GK","TFH2480Z/T","","TFH4525Y/T","","TFH2511Z","","MTZ40JH4","","NTZ068A4LR1B"]
["","Metodă de pornire_","","","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","","Direct","Direct","","Direct","","Direct","","Direct","","Direct"]
["Condensator","Debit de aer","","","m³/h","750","","750","","750","","750","","750","","1400","","1400","1400","","1500","","1500","","1500","","1500"]
["Degivrare","","","","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","","Electric","Electric","","Electric","","Electric","","Electric","","Electric"]
["Încălzitoare de degivrare","W","","","","450","","450","","450","","450","","450","","800","","800","800","","1400","","1400","","1400","","1400"]
["Evaporator","Lungime jet de aer","","","m","","4","","4","","4","","4","","4","","4","","","4","","4","","4","","4","","4"]
["Domeniu de funcţionare","Temperatură cameră frigorifică","","Min.","°C","-5","","-5","","-25","","-25","","-25","","-5","","-25","-25","","-5","","-25","","-5","","-25"]
["","","","Max.","°C","10","","10","","-15","","-15","","-15","","10","","-15","-15","","10","","-15","","10","","-15"]
["Gama de operare","Temperatura din mediul ambiant","","Min.","°C","20","","20","","20","","20","","20","","20","","20","20","","20","","20","","20","","20"]
["","","","Max.","°C","45","","45","","45","","45","","45","","45","","45","45","","45","","45","","45","","45"]
["Agent frigorific","Tip","","","","R-134a","","R-134a","","R-452A","","R-452A","","R-452A","","R-134a","","R-452A","R-452A","","R-134a","","R-452A","","R-134a","","R-452A"]
["","GWP","","","","1430","","1430","","2140","","2140","","2140","","1430","","2140","2140","","1430","","2140","","1430","","2140"]
["Alimentare curent","Tensiune","","","V","220-230","","220-230","","220-230","","220-230","","220-230","","220-230","","230","380-400","","380-400","","380-400","","380-400","","380-400"]
["Alimentare electrică","Fază","","","","1~","","1~","","1~","","1~","","1~","","1~","","1~","3N~","","3N~","","3N~","","3N~","","3N~"]
["Alimentare curent","Frecvenţă","","","Hz","50","","50","","50","","50","","50","","50","","50","50","","50","","50","","50","","50"]