{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Funcţionare silenţioasă","dBA","","36","","41"]
["","","","Scăzut","dBA","","38","","43"]
["","Răcire","","Funcţionare silenţioasă","dBA","","36","","41"]
["","","","Scăzut","dBA","","38","","43"]
["","","","Înalt","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Accesorii standard","Manual de instalare","","","","","Manual de instalare","","Manual de instalare"]
["","Manual de utilizare","","","","","Manual de utilizare","","Manual de utilizare"]
["","Şuruburi","","","","","Şuruburi","","Şuruburi"]
["","Şaibă","","","","","Şaibă","","Şaibă"]
["","Telecomandă fără fir","","","","","Telecomandă fără fir","","Telecomandă fără fir"]
["","Grilaj capac cu blocare","","","","","Grilaj capac cu blocare","","Grilaj capac cu blocare"]
["","Baterie","","","","","Baterie","","Baterie"]
["Sisteme de control","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Racorduri conducte","Lichid","","Dext","mm","","9.52","","9.52"]
["","Gaz","","Dext","mm","","15.88","","15.88"]
["","Drenare","","","","","19.05","","19.05"]
["Putere intrare","Răcire","","Nom.","kW","","0.094","","0.137"]
["","Încălzire","","Nom.","kW","","0.094","","0.137"]
["Sound power level","Răcire","","","dBA","","56","","60"]
["","Încălzire","","","dBA","","56","","60"]
["Dimensiuni","Unitate","","Lățime","mm","","820","","820"]
["","","","Adâncime","mm","","820","","820"]
["","","","Înălțime","mm","","300","","300"]
["Casing","Material","","","","","Oţel galvanizat","","Oţel galvanizat"]
["Greutate","Unitate","","","kg","","39","","39"]
["Ventilator","Debit de aer","Încălzire","Înalt","m³/min","","29.2","","34.0"]
["","","","Scăzut","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Răcire","Scăzut","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Înalt","m³/min","","29.2","","34.0"]
["","","","Funcţionare silenţioasă","m³/min","","17.6","","22.1"]
["","","Răcire","Funcţionare silenţioasă","m³/min","","17.6","","22.1"]
["Panou decorativ","Greutate","","","kg","","4","","4"]
["","Dimensiuni","","Înălțime","mm","","82","","82"]
["","","","Adâncime","mm","","990","","990"]
["","","","Lățime","mm","","990","","990"]
["","Culoare","","","","","Alb","","Alb"]
["Power supply","Phase","","","","","1~","","1~"]
["","Nume","","","","","V1","","V1"]
["","Frecvenţă","","","Hz","","50","","50"]
["","Tensiune","","","V","","220-240","","220-240"]
["Ventilator","Debit de aer","Încălzire","Funcţionare silenţioasă","m³/min","15","","22.1"]
["Putere intrare","Încălzire","","Nom.","kW","0.067","","0.137"]
["","Răcire","","Nom.","kW","0.067","","0.137"]
["Ventilator","Debit de aer","Răcire","Funcţionare silenţioasă","m³/min","15","","22.1"]
["Carcasă","Material","","","","Oţel galvanizat","","Oţel galvanizat"]
["Dimensiuni","Unitate","","Înălțime","mm","265","","300"]
["","","","Lățime","mm","820","","820"]
["","","","Adâncime","mm","820","","820"]
["Greutate","Unitate","","","kg","31","","39"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Scăzut","m³/min","17.6","","26.3"]
["","","Încălzire","Înalt","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Scăzut","m³/min","17.6","","26.3"]
["Nivel de putere sonoră","Răcire","","","dBA","54","","60"]
["","Încălzire","","","dBA","54","","60"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Scăzut","dBA","35","","43"]
["","","","Funcţionare silenţioasă","dBA","32","","41"]
["","Încălzire","","Înalt","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Scăzut","dBA","35","","43"]
["","","","Funcţionare silenţioasă","dBA","32","","41"]
["Racorduri conducte","Lichid","","Dext","mm","9.52","","9.52"]
["","Gaz","","Dext","mm","15.88","","15.88"]
["","Drenare","","","","19.05","","19.05"]
["Panou decorativ","Dimensiuni","","Înălțime","mm","82","","82"]
["","","","Lățime","mm","990","","990"]
["","","","Adâncime","mm","990","","990"]
["","Greutate","","","kg","4","","4"]
["Sisteme de control","Telecomandă cu infraroșii","","","","ARCWLA","","ARCWLA"]
["","Telecomandă cu fir","","","","ARCWB","","ARCWB"]
["Accesorii standard","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Alimentare electrică","Fază","","","","1~","","1~"]
["Alimentare curent","Frecvenţă","","","Hz","50","","50"]
["","Tensiune","","","V","220-240","","220-240"]