{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC073"]
[]
[]
[]
[]
["","","","","BRC073A1"]
["Ambalare","Material","","","Carton_"]
["","Greutate","","kg","0.050"]
["Temperatura din mediul ambiant","Umiditate relativă <","","%","95"]
["","Depozitare","Min.","°C","-20"]
["","","Max.","°C","70"]
["","În timpul funcţionării","Min.","°C","-10"]
["","","Max.","°C","50"]
["Setare de temperatură","Rezoluţie","","°C","1"]
["","Domeniul valorii de referinţă:","Răcire","°C","18-32"]
["","","Încălzire","°C","10-30"]
["Dimensiuni","Unitate integrată","Lățime","mm","220"]
["","","Înălțime","mm","50"]
["","","Adâncime","mm","160"]
["","Unitate","Lățime","mm","120"]
["","","Adâncime","mm","19"]
["","","Înălțime","mm","120"]
["Casing","Capac butoane","","","Nu"]
["","Colour","","","Alb crud"]
["","Operation LED","Colour","","Verde"]
["LCD","Tip","","","Punct plin (160 x 255)"]
["","Lumina de fundal","Culoare","","Alb"]
["","Dimensiuni","Lăţime","mm","68.85"]
["","","Înălţime","mm","43.2"]
["Greutate","Unitate ambalată","","kg","0.348"]
["","Unitate","","kg","0.290"]