{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Nivelul de presiune sonoră","Încălzire","","Înalt","dBA","40","","","","","","45"]
["","","","Funcţionare silenţioasă","dBA","19","","","","","","22"]
["","","","Scăzut","dBA","27","","","","","","33"]
["","Răcire","","Funcţionare silenţioasă","dBA","19","","","","","","21"]
["","","","Scăzut","dBA","24","","","","","","33"]
["","","","Înalt","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Răcire","","Nom.","dBA","32","","","","","","39"]
["Accesorii standard","Manual de instalare","","","","1","","","","","","1"]
["","Manual de utilizare","","","","1","","","","","","1"]
["","Telecomandă fără fir","","","","1","","","","","","1"]
["","Baterii","","","","2","","","","","","2"]
["","Suport telecomandă","","","","1","","","","","","1"]
["","Placă de montare","","","","1","","","","","","1"]
["","Şuruburi de fixare a aparatului interior","","","","2","","","","","","2"]
["","Filtru pentru purificarea aerului din apatit de titan fotocatalitic","","","","2","","","","","","2"]
["Sisteme de control","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Racorduri conducte","Liquid","","OD","mm","6.35","","","","","","6.35"]
["","Gaz","","Dext","mm","9.5","","","","","","9.5"]
["","Drenare","","","","18","","","","","","18"]
["Putere intrare","Răcire","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Încălzire","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Nivel de putere sonoră","Răcire","","","dBA","58","","","","","","59"]
["","Încălzire","","","dBA","58","","","","","","59"]
["Dimensiuni","Unitate","","Lăţime","mm","780","","","","","","900"]
["","","","Adâncime","mm","215","","","","","","215"]
["","","","Înălţime","mm","289","","","","","","298"]
["Carcasă","Culoare","","","","Alb","","","","","","Alb"]
["Greutate","Unitate","","","kg","8","","","","","","11"]
["Power supply","Fază","","","","1~","","","","","","1~"]
["","Frecvenţă","","","Hz","50","","","","","","50"]
["","Nume","","","","V1","","","","","","V1"]
["","Tensiune","","","V","220-240","","","","","","220-240"]
["Note","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Atunci când sunteţi conectat la aparatul exterior al unui multisistem, consultaţi specificaţiile unităţii multi exterioară de conectat.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230 V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Putere intrare","Răcire","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Încălzire","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Carcasă","Culoare","","","","","Alb","Alb","Alb","Alb","Alb","","Alb","Alb","Alb"]
["Dimensiuni","Unitate","","Înălțime","mm","","215","289","215","298","215","","215","298","215"]
["","","","Lățime","mm","","780","780","780","900","900","","900","900","900"]
["","","","Adâncime","mm","","289","215","289","215","298","","298","215","298"]
["Greutate","Unitate","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Debit de aer","Răcire","Înalt","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","","Medie","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Scăzut","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Funcţionare silenţioasă","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Încălzire","Înalt","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","","Medie","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","","Scăzut","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Funcţionare silenţioasă","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Nivel de putere sonoră","Răcire","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Încălzire","","","dBA","","58","58","58","59","59","","59","60","60"]
["Nivelul de presiune sonoră","Răcire","","Înalt","dBA","","40","41","41","45","45","","45","46","46"]
["Nivel de presiune sonoră","Răcire","","Medie","dBA","","32","33","33","","37","","39","","40"]
["Nivelul de presiune sonoră","Răcire","","Scăzut","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Funcţionare silenţioasă","dBA","","19","19","19","19","19","","21","23","23"]
["","Încălzire","","Înalt","dBA","","40","41","41","45","45","","45","47","47"]
["Nivel de presiune sonoră","Încălzire","","Medie","dBA","","34","34","34","","39","","39","","40"]
["Nivelul de presiune sonoră","Încălzire","","Scăzut","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Funcţionare silenţioasă","dBA","","19","19","19","19","19","","22","24","24"]
["Racorduri conducte","Lichid","","Dext","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gaz","","Dext","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Drenare","","","","","18","18","18","18","18","","18","18","18"]
["Sisteme de control","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Accesorii standard","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Alimentare electrică","Nume","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fază","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Alimentare curent","Frecvenţă","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Tensiune","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Debit de aer","Răcire","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Nivelul de presiune sonoră","Răcire","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Debit de aer","Încălzire","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Nivelul de presiune sonoră","Încălzire","","Nom.","dBA","","","34","","39","","","","40"]
["Sisteme de control","Telecomandă cu infraroșii","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Accesorii standard","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Note","","","","","","","","","","","(4) - 240V"]